# This is a Revit shared parameter file.
# Do not edit manually.
*META	VERSION	MINVERSION
META	2	1
*GROUP	ID	NAME
GROUP	1	Dimensions
GROUP	5	Electrical
GROUP	6	Mechanical
GROUP	8	Identity Data
GROUP	10	Electrical - Loads
GROUP	11	Mechanical - Air Flow
GROUP	12	Energy Analysis
GROUP	14	Mechanical - Loads
GROUP	19	Materials and Finishes
GROUP	20	Construction
GROUP	21	Plumbing
GROUP	22	Other
GROUP	23	Green Building Properties
GROUP	24	Constraints
*PARAM	GUID	NAME	DATATYPE	DATACATEGORY	GROUP	VISIBLE
PARAM	aad7c100-5cd6-46de-a224-3bb04707986a	Refrigerant Suction Gas Connection Diameter	PIPE_SIZE		1	1
PARAM	586d6101-4a1e-49a6-9b91-7a3f608c630a	Starter Phase	INTEGER		5	1
PARAM	174cdd01-946e-4909-bf4b-6f7b143344d9	Design Heating Air Flow Maximum	HVAC_AIR_FLOW		11	1
PARAM	3322e901-ca02-42fe-a7f2-db576614a4d7	Compressor Quantity	INTEGER		6	1
PARAM	ced7b602-d099-4061-8fc5-10774f7d8808	Exhaust Fan	YESNO		20	1
PARAM	1f112f03-8d21-4f1b-aec7-a0312d2e3212	Compressor Minimum Outdoor Air Dry Bulb Temperature	HVAC_TEMPERATURE		6	1
PARAM	dc2b6b03-1fa2-4c15-b900-549844bf74f3	Fluid Cooler Water Entering Temperature	PIPING_TEMPERATURE		6	1
PARAM	d3eabb03-7880-47fa-ad1b-11c777fda277	Actual Chilled Water Coil Condensate Drain Flow	PIPING_FLOW		21	1
PARAM	e56f2f04-58ff-4786-9d0e-977ceeea6ac5	Minimum Circuit Current	ELECTRICAL_CURRENT		10	1
PARAM	6d3c6004-dce9-4ccf-9320-148946c8b5bc	Heating Seasonal Performance Factor	NUMBER		12	1
PARAM	65ff6404-5bd1-4d6b-9037-50c1166ef306	Condenser Fan Type	TEXT		6	1
PARAM	137c6e04-d89d-469f-9fa9-b926e1d1104a	Actual Exhaust Air Flow	HVAC_AIR_FLOW		11	1
PARAM	7526e004-50d7-44f2-a613-655dd194f29e	Compressor Voltage	ELECTRICAL_POTENTIAL		5	1
PARAM	6608f604-58c9-4a25-97cf-628d8da4fce5	Supply Fan Number of Poles	NOOFPOLES		5	1
PARAM	73fd6205-40a6-498d-bdd4-9a64a1811962	Cooling Coil 4 Water Entering Temperature	HVAC_TEMPERATURE		6	1
PARAM	987ca005-e391-496b-8440-338a8ef9dff8	Economizer	YESNO		20	1
PARAM	e14be705-93dc-47ed-b16f-8abe50aa8835	Cooling Coil 4 Entering Dry Bulb Temperature	HVAC_TEMPERATURE		6	1
PARAM	24452f06-fde6-42b5-8cd5-8d44e579f382	Coefficient of Performance	NUMBER		12	1
PARAM	11acb006-afbf-43ef-b35a-7313f3e7ea18	Filter 5 Face Area	AREA		11	1
PARAM	cdafdf06-7a58-4c1f-820f-264a9d5af216	Serial Number	TEXT		8	1
PARAM	d449ed06-9ce0-425b-9f6c-a75630dafad0	Equivalent Direct Radiation	AREA		6	1
PARAM	32294a07-cce7-49df-b0f8-ca6a05ae52e3	Flue Diameter	HVAC_DUCT_SIZE		1	1
PARAM	4d535507-0644-4e78-b512-092e1133a72e	Return Fan External Static Pressure	HVAC_PRESSURE		6	1
PARAM	0b538507-88db-4d93-9a9c-6903adcc42a6	Power Factor	NUMBER		5	1
PARAM	b55e9d07-a564-4427-95a6-b719bdbad4cf	Fluid Cooler Fan Power	ELECTRICAL_POWER		10	1
PARAM	a588f307-7b30-415e-bd0f-4cf681c73432	Actual Fan Powered Box Primary Air Flow	HVAC_AIR_FLOW		11	1
PARAM	54394608-13c1-436f-b885-1f0d3d907b9a	Cooling Coil 4 Water Leaving Temperature	HVAC_TEMPERATURE		6	1
PARAM	ad17b208-8987-4c58-b5d3-2b5bac288248	Return External Static Pressure	HVAC_PRESSURE		11	1
PARAM	0e85ef09-32e5-4e7d-9cda-229002bd77b7	Heating Coil Description	TEXT		6	1
PARAM	cbedff09-2ec3-4a5a-b74f-0de2518335d6	Heating Coil 4 Entering Dry Bulb Temperature	HVAC_TEMPERATURE		6	1
PARAM	ab36840a-2d40-45b5-b807-6c627f91ad16	Cooling Coil 3 Air Pressure Drop	HVAC_PRESSURE		6	1
PARAM	ba7fa50a-a7d8-430f-80e0-41f463aea9f4	Typical Comment	TEXT		8	1
PARAM	b4ebb30a-ee36-4c1b-b009-490b73eaa4ea	Heating Coil 2 Entering Wet Bulb Temperature	HVAC_TEMPERATURE		6	1
PARAM	d0bb040b-352d-4450-8a2d-20db34ca3783	ARI Number	TEXT		8	1
PARAM	686c3e0b-1843-4a9c-ab3b-e6e4f0156c5a	Refrigerant Suction Gas Connection 2 Diameter	PIPE_SIZE		1	1
PARAM	5f92500d-9a36-49ef-a00a-3e681a641d86	Waterside Economizer Cooling Entering Wet Bulb Temperature	HVAC_TEMPERATURE		11	1
PARAM	895ddb0d-6098-42d1-8167-4b1e021de954	Energy Efficiency Rating	NUMBER		12	1
PARAM	67159b0e-2541-424b-b1a1-7c46a09e9809	Electric Heat Description	TEXT		6	1
PARAM	2fab1c0f-f787-4343-a149-c03098bd1098	Control Protocol	TEXT		8	1
PARAM	3f785a0f-4e3d-47a3-9523-33828f3efed5	Cooling Coil Sensible Cooling Capacity	HVAC_COOLING_LOAD		6	1
PARAM	f513b80f-aed9-476f-882b-7bdd70ff236b	Pump Power	ELECTRICAL_POWER		10	1
PARAM	b3b5a310-96b3-451e-bc69-b57d2d49f50b	Ventilation Air Connection Height	HVAC_DUCT_SIZE		1	1
PARAM	723ed810-f04f-4fa3-b9c2-0bf9365ad919	Equipment Finish	MATERIAL		19	1
PARAM	daa4ef10-0de4-4af9-8b32-1cf6800fac5a	External Static Pressure	HVAC_PRESSURE		14	1
PARAM	d4011d11-27cd-4211-8b71-0c24d8265ff6	Sound Attenuator 2 Description	TEXT		6	1
PARAM	6223c911-5822-4a43-a118-a9d0b3546ade	Filter 3 Air Pressure Drop	HVAC_PRESSURE		11	1
PARAM	a4034013-c49d-4f10-b756-0d74b6e18635	Chilled Water 2 Leaving Temperature	PIPING_TEMPERATURE		6	1
PARAM	14a4a813-1981-4853-a05c-0c553b8be5a1	LEED Credit	TEXT		23	1
PARAM	4cd3ab13-eb96-4ec5-b874-1ea2f7a7ab8e	Rated Load Current	ELECTRICAL_CURRENT		10	1
PARAM	132cc913-b3ae-45e8-a6e4-f82c6c1a57bf	Condenser Relief Valve Connection Diameter	PIPE_SIZE		1	1
PARAM	18db0714-17eb-427e-990e-cf0d0b66171c	Return Fan Total Static Pressure	HVAC_PRESSURE		6	1
PARAM	562daa14-c746-43f2-8ff3-0b04ee1c7d0a	Cooling Coil Description	TEXT		6	1
PARAM	c671aa14-17bc-4c2b-a75f-826a60122a92	Cooling Coil Total Cooling Capacity	HVAC_COOLING_LOAD		6	1
PARAM	aecd0015-283f-4d77-a40e-1a7bd0dc9559	Filter 3 Efficiency	TEXT		11	1
PARAM	5a002a15-059a-420d-863d-7d3a1395ba88	Return Fan Quantity	NUMBER		6	1
PARAM	e6806c15-bb41-4cfb-bebf-8cdd1f034805	Return Fan Minimum Circuit Current	ELECTRICAL_CURRENT		10	1
PARAM	39d09315-298f-4c65-a20d-367885b6adbb	Hot Gas Bypass 2 Connection Diameter	PIPE_SIZE		1	1
PARAM	50410016-8582-4923-9bb4-a8589146ab0e	Sound Radiated Noise Criteria	NUMBER		6	1
PARAM	51ce2e16-74ec-4e63-b1ff-b4aa4b976058	Compressor 2 Quantity	INTEGER		6	1
PARAM	2402fa17-c9a1-4e45-b97d-5f29dba308cb	Cooling Coil 4 Glycol Percentage	NUMBER		6	1
PARAM	67470118-e2b5-4c5a-b7c8-31a98da5423a	Design Ambient Winter Dry Bulb Temperature	HVAC_TEMPERATURE		12	1
PARAM	628e2c18-822d-4140-b3f9-dfe05d253eb7	Heating Coil 5 Face Velocity	HVAC_VELOCITY		6	1
PARAM	24594f19-d09e-4f4d-8bfb-18c058b02158	PreFilter Quantity	INTEGER		11	1
PARAM	3cd05019-60c6-435d-a1de-2cd5ad886a40	Design Return Air Flow Maximum	HVAC_AIR_FLOW		11	1
PARAM	99489c19-b7ca-45a8-998f-45252affe51e	Low Pressure Gas Equalizer Connection Diameter	PIPE_SIZE		1	1
PARAM	9555fd19-9636-4f95-8dca-d70644e6d12c	Actual Heating Water 2 Flow	PIPING_FLOW		6	1
PARAM	a763031a-b78f-49c2-906f-aa85a7102aae	Cooling Coil 2 Total Cooling Capacity	HVAC_COOLING_LOAD		6	1
PARAM	0151041a-8ea0-4bdb-a2f0-683d7f816212	Steam Pressure	PIPING_PRESSURE		21	1
PARAM	a5cd291a-1ad3-466c-890d-012b68fa1a7a	Fluid Cooler Water Pressure Drop	PIPING_PRESSURE		6	1
PARAM	cb56631a-26c7-42b5-a1cd-600788e3af28	Heating Coil 5 Water Leaving Temperature	HVAC_TEMPERATURE		6	1
PARAM	6ca6701a-a2ef-4211-9042-600bbbb698a7	Waterside Economizer Water Leaving Temperature	PIPING_TEMPERATURE		6	1
PARAM	f151021b-8c09-46d7-8d72-f4ec2f192452	Design Ambient Summer Wet Bulb Temperature	HVAC_TEMPERATURE		12	1
PARAM	c338041b-dc4e-45ad-8677-2de49cbcb64d	Heating Coil 3 Entering Wet Bulb Temperature	HVAC_TEMPERATURE		6	1
PARAM	0b2afe1b-09e8-4ba0-89c9-f4c8284409c7	Design Fluid Cooler Water Flow	PIPING_FLOW		6	1
PARAM	bfbb6e1c-3714-4f69-beb7-29c5a113337d	Return Fan Full Load Current	ELECTRICAL_CURRENT		10	1
PARAM	64b7e91c-890f-428b-8122-a0e06096f74c	Heating Coil 5 Refrigerant Saturated Suction Temperature	HVAC_TEMPERATURE		6	1
PARAM	d2a4461d-5197-4fb8-ad8c-2c9ce40c6b5d	Cooling Coil 3 Glycol Type	TEXT		6	1
PARAM	0168881d-60ad-4f20-b0a5-ac47b70aede7	Economizer Enthaply Limit	NUMBER		6	1
PARAM	beb3b21d-21d3-4c09-8245-0f3b30319a6a	Fluid Cooler Number of Feeds	INTEGER		6	1
PARAM	ef90f11d-b3aa-49be-bdac-1e8990eaadae	Heat Pump Source Leaving Temperature for Heating	HVAC_TEMPERATURE		6	1
PARAM	898ef91d-3a9f-4ffe-87dc-43791d623313	Chilled Water Entering Temperature	PIPING_TEMPERATURE		6	1
PARAM	9afa161e-de87-460a-8066-a10e1587e7e9	Design Total Power	ELECTRICAL_POWER		10	1
PARAM	8673781e-e7a4-4775-b198-f9930f0483d3	Filter 3 Description	TEXT		11	1
PARAM	3e09961e-72c6-49f4-beea-bbac4f4adc24	Supply Fan Full Load Current	ELECTRICAL_CURRENT		10	1
PARAM	4b87641f-59e7-4bf9-b4d2-3bfac6e74994	Economizer Air Pressure Drop	HVAC_PRESSURE		11	1
PARAM	a4631c20-c244-4e68-9f73-393644e2d4e3	Fluid Cooler Water Leaving Temperature	PIPING_TEMPERATURE		6	1
PARAM	2a973320-7fb0-40d8-97da-543cb85dae16	Low Temperature Heating Standard Rating Capacity	HVAC_HEATING_LOAD		14	1
PARAM	779c4020-8034-4de4-9c60-32747e2954b1	Filter 4 Description	TEXT		11	1
PARAM	a7b0ca20-b7ee-46d8-b79e-3151def4d4c2	Damper Air Flow	HVAC_AIR_FLOW		11	1
PARAM	9ef7e620-4e99-49f2-b931-05d278850797	Heating Coil 5 Entering Wet Bulb Temperature	HVAC_TEMPERATURE		6	1
PARAM	918ec421-9fc6-4ede-9fd3-de77e9ee11ec	PreHeating Entering Dry Bulb Temperature	HVAC_TEMPERATURE		11	1
PARAM	a6368922-770d-4056-b47d-aea85ea3b8cf	Electric Heat Apparent Load	ELECTRICAL_APPARENT_POWER		10	1
PARAM	4ae38c22-7f31-4683-a5cc-437e4b90d44b	Design Air Flow Minimum	HVAC_AIR_FLOW		11	1
PARAM	04631523-ece5-442c-9c23-5d14dc6b4472	Actual Pump Water Flow	PIPING_FLOW		21	1
PARAM	3d8a4923-98a6-4d64-86fe-af81762285d4	Pump HP	ELECTRICAL_POWER		10	1
PARAM	48145323-93a2-4b1a-89c4-b69d480ad891	PreHeating Coil Row Count	NUMBER		6	1
PARAM	f4d08723-fd59-4ae6-b1ea-2e2bca0b23db	Manifold Output 2 Diameter	PIPE_SIZE		1	1
PARAM	20b48f24-3d25-4941-ab72-ba9edcb96e75	Air In Connection Height	HVAC_DUCT_SIZE		1	1
PARAM	1a95a724-2e55-4384-addf-716888231f65	Heating Coil 2 Air Pressure Drop	HVAC_PRESSURE		6	1
PARAM	98dbc924-742c-4be2-8cbf-7222da5893de	Filter 4 Face Velocity	HVAC_VELOCITY		6	1
PARAM	bd178a25-991b-4880-a3b5-4c4dcfb2a99b	Steam Connection 2 Diameter	PIPE_SIZE		1	1
PARAM	0f8e9425-41bf-4876-a9d1-55a918763e2a	Cooling Coil 5 Entering Wet Bulb Temperature	HVAC_TEMPERATURE		6	1
PARAM	39c6a725-114a-4089-863d-3d34859f7f63	Cooling Coil 2 Air Pressure Drop	HVAC_PRESSURE		6	1
PARAM	88e7c725-b1ed-4ab1-9677-d3f871c7a5f2	Cooling Coil 4 Water Pressure Drop	PIPING_PRESSURE		6	1
PARAM	74440528-fbaf-4b0a-82f7-ab3df4ae4f00	Steam Humidifier Flow for Schedule	NUMBER		21	1
PARAM	70e61628-cbd8-406e-b3a5-f90632a229b3	Waterside Economizer Cooling Coil Sensible Cooling Capacity	HVAC_COOLING_LOAD		14	1
PARAM	6c63a328-d517-4259-91fb-b226af0144ae	Supply Fan Quantity	INTEGER		6	1
PARAM	f932ab28-2916-4771-a511-28c275f01c42	Manufacturer Metadata	TEXT		8	0
PARAM	072cc92b-760f-4849-a712-e0d4603bcf9a	Evaporator Coil Face Area	AREA		1	1
PARAM	11e64c2c-8d59-4161-a22f-f8402804965e	Nominal Cooling Capacity	HVAC_COOLING_LOAD		14	1
PARAM	be15482d-8b48-4396-93d8-2f7eeaea5e8c	Actual Supply Air Connection 3 Flow	HVAC_AIR_FLOW		11	1
PARAM	a381ef2d-0522-497d-bf3c-edcd78351e3d	Heating Coil 2 Glycol Percentage	NUMBER		6	1
PARAM	69bdf42d-6913-4831-8f89-2d11928e77e3	Operating Weight	FORCE		8	1
PARAM	cb4bfe2d-0aba-4475-9629-20379916d128	Return Fan Type	TEXT		6	1
PARAM	a369212e-0761-4dfa-bc04-cff777ddb79f	NEMA Receptacle	TEXT		5	1
PARAM	c11b572e-4890-45c6-a255-c7b48e7f9b48	Exhaust Air Connection Height	HVAC_DUCT_SIZE		1	1
PARAM	9cbf592e-b48d-4b68-a345-30a83cfb8fd4	Heating Coil Water Entering Temperature	HVAC_TEMPERATURE		6	1
PARAM	af4ff52f-8d1c-43cc-a8eb-75f1c6653e53	Enthalpy Wheel Number of Poles	NOOFPOLES		5	1
PARAM	4c112130-fef6-4696-a33e-80c1ead96fbb	Cooling Coil 4 Total Cooling Capacity	HVAC_COOLING_LOAD		6	1
PARAM	bb5d8d30-ef84-4f68-9ae1-c9092a7509e8	Supply Fan Total Static Pressure	HVAC_PRESSURE		6	1
PARAM	ed6d8f30-f87e-459f-b085-54bb03d7e0ab	Heating Coil Refrigerant Saturated Suction Temperature	HVAC_TEMPERATURE		6	1
PARAM	9993b730-9dc3-4f02-a78f-445b59bdfc0a	Evaporator Coil Row Count	NUMBER		1	1
PARAM	4076ed30-8e95-47ba-afdf-bdbc5d1cb9fa	Exhaust Fan Disconnect	TEXT		5	1
PARAM	57e12131-f42d-4f5c-b9f9-ca0d66a04dfd	Heating Coil 4 Entering Wet Bulb Temperature	HVAC_TEMPERATURE		6	1
PARAM	92ed7a31-adae-4e8d-bbb6-f23c0cb09b6a	Electric Heat	YESNO		20	1
PARAM	53680c32-a704-4904-8509-6bf7de8e775f	Cooling Coil 5 Fin Density	NUMBER		6	1
PARAM	e30d0e32-ac04-4063-9666-0c6db3adcb81	Apparent Load Circuit 1	ELECTRICAL_APPARENT_POWER		10	1
PARAM	47dc5633-5872-46d7-8bdb-45417098a233	Supply Air Connection Width	HVAC_DUCT_SIZE		1	1
PARAM	c4618c33-d47d-4c7a-a2de-adae18ff04d0	Exhaust Air Connection Diameter	HVAC_DUCT_SIZE		1	1
PARAM	2fe0a033-ae1e-4e62-9ea9-f08bd99bfe26	Interior Finish	TEXT		19	1
PARAM	4c8bb433-a6a5-4d69-ab88-ebdac9f71237	Maximum Vertical Refrigerant Pipe Length Above Unit	LENGTH		6	1
PARAM	e4f14a34-9c56-4f6c-b17a-18c67711daf7	Actual Chilled Water Flow	PIPING_FLOW		6	1
PARAM	d20d9934-4fd5-47fb-9b73-184e06f8e427	Suction Relief Valve Connection Diameter	PIPE_SIZE		1	1
PARAM	ad7dd234-3b02-4c00-b175-fa3dc59e5885	Filter 5 Face Velocity	HVAC_VELOCITY		6	1
PARAM	45279535-09da-4a72-9428-d844ac202e7f	Condenser Water Connection Diameter	PIPE_SIZE		1	1
PARAM	a9c00836-3edb-4ac9-bd2f-c728f33f87ff	Heat Pump Source Leaving Temperature for Cooling	HVAC_TEMPERATURE		6	1
PARAM	084b5736-1272-47a3-b9cd-2ffbd2eb3f20	Combination Ratio	NUMBER		6	1
PARAM	47d66636-ff53-45f5-802e-59c67c70e611	Heating Coil 3 Air Pressure Drop	HVAC_PRESSURE		6	1
PARAM	cc55b436-ac6c-48fd-83cc-b964cd6fae74	Gas Heater Air Pressure Drop	HVAC_PRESSURE		11	1
PARAM	6fe5e036-5e04-4184-a186-207503c49b65	Return Fan Phase	NOOFPOLES		5	1
PARAM	cc8d0337-203e-4b5f-83ee-96471e1172e6	Include Clearance	YESNO		24	1
PARAM	73683b37-dc3f-492d-926c-625870b0a4f0	Actual Supply Air Connection 1 Flow	HVAC_AIR_FLOW		11	1
PARAM	2c437b37-e51e-434a-840f-adf0f3480b9a	Design Cooling Air Flow Minimum	HVAC_AIR_FLOW		11	1
PARAM	80f29237-0963-42d4-b9fa-11ed00f414a6	Compressor Number of Poles	NOOFPOLES		5	1
PARAM	bebe8438-711e-408e-8dab-f04a0006302a	Power Source Type	TEXT		8	1
PARAM	225ef538-a72d-4360-aa6a-bd842d439f54	Filter 4 Air Pressure Drop	HVAC_PRESSURE		11	1
PARAM	53770139-9d6b-4ad4-bb48-a24f483ee8be	Return Air Connection Width	HVAC_DUCT_SIZE		1	1
PARAM	3a082139-17a9-4400-83f6-e3b48113762b	Heating Coil Air Pressure Drop	HVAC_PRESSURE		6	1
PARAM	1411b139-76e1-4776-8ea7-48530e9c21cc	Return Fan Description	TEXT		6	1
PARAM	9e39c839-4591-4308-ace3-115ffb576245	Waterside Economizer Cooling Coil Total Cooling Capacity	HVAC_COOLING_LOAD		14	1
PARAM	746df239-7cfa-4c52-9d7d-269703608c6a	Actual Vertical Refrigerant Pipe Length Above Unit	LENGTH		6	1
PARAM	b986383a-ba28-4a39-8902-efab5d934725	Heating Coil 3 Water Pressure Drop	PIPING_PRESSURE		6	1
PARAM	b5ae633a-f577-47b4-992c-b78af1969535	Design Primary Air Flow Minimum	HVAC_AIR_FLOW		11	1
PARAM	da3a8e3a-61b4-49ce-9bd9-9806d5219de7	Filter 2 Height	LENGTH		1	1
PARAM	e9f6b03a-656c-4532-86c2-267a3a65a47f	Cooling Coil 2 Water Entering Temperature	HVAC_TEMPERATURE		6	1
PARAM	40bad03a-3d55-4eb4-9264-7b0a1bb59b67	Induced Air Connection Height	HVAC_DUCT_SIZE		1	1
PARAM	5d14063b-8a75-445f-896e-73a1d162151b	Heating Coil 2 Fin Density	NUMBER		6	1
PARAM	b7177d3b-99ec-44fe-a702-27efbbeadbef	Filter Length	LENGTH		1	1
PARAM	3e008c3b-6193-4926-9718-a7dacada8eab	Curb Wall Thickness	LENGTH		1	1
PARAM	62a48f3b-b0d8-49dd-a2b4-cf9d155aa543	Cooling Coil Row Count	NUMBER		6	1
PARAM	bc48153c-0e6a-49db-949c-02bc58e87eb4	Actual Total Power	ELECTRICAL_POWER		10	1
PARAM	2b1a243c-8c74-4242-9816-20db55f69fb9	Cooling Coil 5 Leaving Dry Bulb Temperature	HVAC_TEMPERATURE		6	1
PARAM	986e2d3c-6b09-4e80-bfe0-4667f039391f	Cooling Coil 4 Leaving Dry Bulb Temperature	HVAC_TEMPERATURE		6	1
PARAM	0fb0493c-02e3-4b54-9ce4-512e10acabcb	Minimum Ambient Temperature	HVAC_TEMPERATURE		6	1
PARAM	917b643c-c589-4c7d-ae68-63ecb324e6fc	Cooling Coil Fin Density	NUMBER		6	1
PARAM	66f7253d-92e2-47eb-925e-06d3651d5fa5	Cooling Tower Fan HP	ELECTRICAL_POWER		10	1
PARAM	6988453d-7889-4ae9-b888-e02089f00dac	Heating Coil 2 Water Pressure Drop	PIPING_PRESSURE		6	1
PARAM	d946753d-acc8-40e5-84ce-71065641e547	High Pressure Gas Equalizer Connection Diameter	PIPE_SIZE		1	1
PARAM	d1c6583e-3179-4023-a373-49081af40905	Cooling Coil 5 Entering Dry Bulb Temperature	HVAC_TEMPERATURE		6	1
PARAM	2e54663e-ccbc-4ce3-8d2a-bb18c8907f76	Cooling Coil 2 Fin Density	NUMBER		6	1
PARAM	a3a1de3e-ff98-464d-8d0d-6ec936f6b39b	Filter Height	LENGTH		1	1
PARAM	f0cff73e-a02b-44ab-a951-3f1431584e18	Heating Nominal Input Power	ELECTRICAL_POWER		10	1
PARAM	ddfe3740-b0ac-4b04-be3a-28b2aa144972	Compressor Variable Frequency Drive	YESNO		6	1
PARAM	11595040-ba0f-48b0-beec-0b497a80f1bd	Induced Air Connection Width	HVAC_DUCT_SIZE		1	1
PARAM	d41a7840-f88a-4b23-8203-a5837c2f02d7	Heating Coil 2 Refrigerant Saturated Suction Temperature	HVAC_TEMPERATURE		6	1
PARAM	78f0af40-2daa-4e11-b802-cdb915e351a0	PreHeating Coil Water Pressure Drop	PIPING_PRESSURE		6	1
PARAM	29c4bb40-f77c-446e-9c58-4e723ca303dd	Heating Coil 4 Water Entering Temperature	HVAC_TEMPERATURE		6	1
PARAM	818e1441-9dd2-43a2-a604-c019dab99974	Cooling Coil 5 Sensible Cooling Capacity	HVAC_COOLING_LOAD		6	1
PARAM	63372841-100d-47cb-868c-0558228b49a3	Equipment Type	TEXT		8	1
PARAM	16943441-0138-4726-971d-ab7bf34858e5	Exhaust Fan Full Load Current	ELECTRICAL_CURRENT		10	1
PARAM	5dabce42-a666-4644-b6b8-ce339a600de5	Design Heating Water Flow	PIPING_FLOW		6	1
PARAM	41cc0143-9d79-4339-8264-5eb74792b2d3	Heating Coil Entering Wet Bulb Temperature	HVAC_TEMPERATURE		6	1
PARAM	347f9e43-93e1-44c4-a095-f34b117587e9	Filter Depth	LENGTH		1	1
PARAM	a33af543-3cb7-4027-89d3-4fffcfeca6ee	Design Pressure	TEXT		22	1
PARAM	32574b44-e79f-47d1-ad83-04148b477e1f	Heating Coil 4 Description	TEXT		6	1
PARAM	af408144-920c-41a1-97c6-3465476aeddb	Heating Coil 4 Actual Flow	PIPING_FLOW		6	1
PARAM	110fb944-3a5d-43ec-815f-13f867c1a32b	Return Fan Power	ELECTRICAL_POWER		10	1
PARAM	761d2545-3896-435f-bdd4-c604ed6d3f67	Ultraviolet Lights Apparent Load	ELECTRICAL_APPARENT_POWER		10	1
PARAM	b73d3546-19a8-49ea-8132-91cf992ca33a	Design Supply Air Flow Maximum	HVAC_AIR_FLOW		11	1
PARAM	f1f03f47-05f3-40c8-8848-d288f73d89b3	Air Out Connection Height	HVAC_DUCT_SIZE		1	1
PARAM	6e5fc847-dbc0-4b9a-9791-059a87177fe0	Gas Connection Diameter	PIPE_SIZE		1	1
PARAM	84d8dd47-760e-4183-b216-b57f447052cc	Cooling Coil 3 Water Entering Temperature	HVAC_TEMPERATURE		6	1
PARAM	a4c0ff47-e3cb-46c0-bee6-6bf1529292d0	Cooling Tower Fan Power	ELECTRICAL_POWER		10	1
PARAM	39cfc448-8bb5-4da9-9da8-cc3c9739e2cd	Primary Air Connection Width	HVAC_DUCT_SIZE		1	1
PARAM	5e186a49-4683-47ac-8df3-ba16b30010bc	Supply Fan Locked Rotor Current	ELECTRICAL_CURRENT		10	1
PARAM	f0463c4a-233e-4fc6-b949-a2966bccd748	Cooling Coil 2 Entering Dry Bulb Temperature	HVAC_TEMPERATURE		6	1
PARAM	9ef3af4a-777f-4865-b52f-cde3428e6e2b	Actual Condensate Drain Flow	PIPING_FLOW		6	1
PARAM	34ce164b-2f26-4400-96dc-875cb495f585	Actual PreHeating Water Flow	PIPING_FLOW		6	1
PARAM	db212a4b-10f6-4cbe-a61b-0ad178a43535	Ambient Wet Bulb Temperature	HVAC_TEMPERATURE		11	1
PARAM	68ee364b-1d63-405e-80b0-3c3b260b7752	Manifold Output Diameter	PIPE_SIZE		1	1
PARAM	abcc4c4b-b817-4daa-b720-794ba4544c78	Area Served	TEXT		8	1
PARAM	5fcdc84b-d3ad-47e6-a9f6-76e5a2a336de	Compressor Minimum Circuit Current	ELECTRICAL_CURRENT		10	1
PARAM	0b79124c-7300-4218-bee7-dba9817a7f28	Chilled Water 2 Connection Diameter	PIPE_SIZE		1	1
PARAM	b0a87b4c-6cf1-42b6-b468-8cb37346baa1	Supply Fan Phase	NOOFPOLES		5	1
PARAM	e4167c4c-7c07-4086-a21c-810f8aefe07b	Cooling Coil 2 Leaving Wet Bulb Temperature	HVAC_TEMPERATURE		6	1
PARAM	21578e4c-b262-4e35-8c76-5ff03320611e	Manifold Input 1 Diameter	PIPE_SIZE		1	1
PARAM	21ca364d-bfca-408f-b3a3-7d40d0200e1e	Supply Fan Voltage	ELECTRICAL_POTENTIAL		5	1
PARAM	4a59b34d-394e-49a2-b93b-5596ed6cbbf2	Gas Heat Turndown	TEXT		14	1
PARAM	507b374e-b423-463c-8cc6-9bc5b1568212	Pump Speed	NUMBER		6	1
PARAM	f4a7854e-af78-4da1-ac1c-7e46a46e1fd7	Actual Heater Gas Flow	PIPING_FLOW		6	1
PARAM	5a1f4e4f-8f10-4e75-bdcc-cde05d0a2b85	Actual Return Air Flow	HVAC_AIR_FLOW		11	1
PARAM	a5bba84f-fb98-4610-b22f-d580b21d0ed5	Heating Coil Sensible Heating Capacity	HVAC_HEATING_LOAD		6	1
PARAM	f516d24f-701a-4655-8e1f-1ed5266dff66	Hot Gas Bypass Connection Diameter	PIPE_SIZE		1	1
PARAM	11e48750-a7e6-4d33-a3b9-8c89eb64ede5	Enthalpy Wheel Description	TEXT		6	1
PARAM	a24ebc50-8568-42d0-a3c5-b3b0272e2c74	Supply Total Static Pressure	HVAC_PRESSURE		11	1
PARAM	d140c550-3764-4ee6-b996-54ecd1fa38d5	Heating Coil Fin Density	NUMBER		6	1
PARAM	015b0551-7942-49f6-adc3-423b4519f3f1	Induced Air Connection Diameter	HVAC_DUCT_SIZE		1	1
PARAM	093a2051-8c2e-4c25-bd02-e0d58ba02103	Heating Coil 3 Water Leaving Temperature	HVAC_TEMPERATURE		6	1
PARAM	6a596a51-8abe-4038-b0c8-a561522bf90c	Ambient Dry Bulb Temperature	HVAC_TEMPERATURE		11	1
PARAM	81a88351-bd0b-4911-b851-13775f1a16af	Compressor Apparent Load	ELECTRICAL_APPARENT_POWER		10	1
PARAM	97319351-9afa-4aea-b422-c6429c1d3254	Actual Fan Powered Box Induced Air Flow	HVAC_AIR_FLOW		11	1
PARAM	0b05b251-9f3c-47ad-a30f-ff12766b748d	Steam Boiler Water Capacity	VOLUME		6	1
PARAM	72933452-fe6c-4184-b133-7a4c634a5954	Condenser Fan HP	ELECTRICAL_POWER		10	1
PARAM	00948a52-e10d-48fa-897b-41fbc6ca122e	Enthalpy Wheel Frequency	ELECTRICAL_FREQUENCY		5	1
PARAM	9a557053-ec15-4f01-8fc2-f605f91d0b3b	Filter 3 Face Velocity	HVAC_VELOCITY		6	1
PARAM	11be8753-3808-4799-bb18-bb0ce40491d3	Evaporator Leaving Temperature	PIPING_TEMPERATURE		6	1
PARAM	42e61154-a5a7-42f0-b597-17dc3c5e3c2e	Point of Shipment	TEXT		8	1
PARAM	d3cf3254-6e31-448d-a263-d144a5cd31f2	Evaporator Diameter	LENGTH		1	1
PARAM	17d53254-a00a-429c-b291-5d6422428843	Makeup Water Flow	PIPING_FLOW		21	1
PARAM	56d0c854-1a60-489d-9755-6a4d7e71f882	Heat Pump Coil Row Count	NUMBER		6	1
PARAM	462df454-3bc1-4bba-b61d-82b959d0b314	Heating Coil Entering Dry Bulb Temperature	HVAC_TEMPERATURE		6	1
PARAM	dd9e2f55-ae7f-4b6e-bc00-9ff08b444527	Filter 4 Size	TEXT		11	1
PARAM	2caf3855-d401-4ac2-b552-7f5270487283	Demand Control Ventilation	YESNO		11	1
PARAM	09dbb055-8554-400c-81d7-51cc5cd2d523	Filter 5 Air Pressure Drop	HVAC_PRESSURE		11	1
PARAM	3370db55-feb6-4f1e-8f90-deaa54a9283f	Branch Quantity	INTEGER		6	1
PARAM	7f023f56-c3a9-44b0-adb2-69272925f1c7	Heating Coil 5 Total Heating Capacity	HVAC_HEATING_LOAD		6	1
PARAM	97375956-f0b4-4219-8ce3-54bf43caefda	Heating Coil 2 Leaving Wet Bulb Temperature	HVAC_TEMPERATURE		6	1
PARAM	610e7056-8cce-4714-a503-0a6757e843c6	Cooling Coil 3 Face Velocity	HVAC_VELOCITY		6	1
PARAM	c801a656-e896-4b07-9d7b-17e8eb3a911d	Design Condenser Flow	PIPING_FLOW		6	1
PARAM	5928cf56-a223-41ab-ab83-1d7be2322cda	Heating Coil 4 Fin Density	NUMBER		6	1
PARAM	de8f3857-ed90-4510-9756-9a43a9bbc01a	Electric Heat Capacity	HVAC_HEATING_LOAD		14	1
PARAM	0d933857-207b-41aa-963b-b1561d4cd707	Oil Connection Diameter	PIPE_SIZE		1	1
PARAM	35610458-1c22-4f50-906e-6fbc3415aa8b	Heating Coil 5 Glycol Percentage	NUMBER		6	1
PARAM	3c61d358-fb91-49fc-8015-68a7fc1d3b31	Enthalpy Wheel Disconnect	TEXT		5	1
PARAM	ba580659-d6d2-4256-bdf4-99d3c9d8d44f	Maximum Rated Over Protection Device	ELECTRICAL_CURRENT		5	1
PARAM	e91a2159-dc0e-472b-928c-6b8a6d47b626	Electric Heat Voltage	ELECTRICAL_POTENTIAL		5	1
PARAM	3760bd59-674c-47a2-9737-3d7fed8fbbe8	PreHeating Leaving Wet Bulb Temperature	HVAC_TEMPERATURE		11	1
PARAM	bc5ae259-f49a-41dc-a148-e7bc613b3a16	Waterside Economizer Cooling Coil Description	TEXT		6	1
PARAM	a1c4f25a-1260-41a5-bac8-97556a57b236	Apparent Load	ELECTRICAL_APPARENT_POWER		10	1
PARAM	3e8bcc5c-b0c2-4e09-9e32-8069c85af83a	Style	TEXT		8	1
PARAM	2d8f5d5d-0426-4d7d-9692-d3e7ea3d90ff	Heating Coil Water Leaving Temperature	HVAC_TEMPERATURE		6	1
PARAM	ab0e8a5d-e0f1-4eb0-82ae-298a98c158c2	Throw Distance Medium Velocity	LENGTH		11	1
PARAM	1d0d915d-3d68-41dc-b137-682a21cdbcf3	Return Fan Locked Rotor Current	ELECTRICAL_CURRENT		10	1
PARAM	4a1b0e5e-e593-4599-9512-315a54cf43e6	Economizer Dry Bulb Limit	HVAC_TEMPERATURE		6	1
PARAM	a09ccf5e-8773-4e9b-8064-3078b2131430	Return Air Connection Height	HVAC_DUCT_SIZE		1	1
PARAM	99c9455f-1a87-45a6-8d69-cf29875ad07e	Cooling Coil 3 Actual Flow	PIPING_FLOW		6	1
PARAM	3005c45f-d638-4dd1-8c2c-3334a6b4d13a	Cooling Coil 2 Row Count	NUMBER		6	1
PARAM	e8aef95f-531e-4107-b6fd-d5c5378b4029	Exhaust Fan Description	TEXT		6	1
PARAM	d2c21560-88e9-483c-a767-291a704ac553	Ultraviolet Lights Phase	NOOFPOLES		5	1
PARAM	a156c860-2383-4987-878a-894522e20699	Actual Hot Water Flow	PIPING_FLOW		6	1
PARAM	98f36961-e218-427b-8045-365dc0ce8900	Design Air Flow Maximum	HVAC_AIR_FLOW		11	1
PARAM	56780b62-88ff-4b79-8abe-46a3dfb513f8	Ventilation Air Flow Range	TEXT		11	1
PARAM	c28d5562-063a-4836-8e85-1f2657b30e37	Heating Coil 4 Glycol Type	TEXT		6	1
PARAM	86745a62-4e9c-4c0d-9af7-f64f0711c0f1	Filter 2 Face Area	AREA		11	1
PARAM	87319162-182d-4198-856f-da8ee80d8cc1	Heat Pump Coil Face Velocity	HVAC_VELOCITY		6	1
PARAM	7febb362-3622-4b24-a1c2-4fe805dad559	Copyright ©	TEXT		8	1
PARAM	305fba62-607c-478d-afcd-2ae2b9e6b286	Waterside Economizer Cooling Leaving Wet Bulb Temperature	HVAC_TEMPERATURE		11	1
PARAM	c8bc5d63-50d1-4b03-ad62-5b8a7d5935bc	PreHeating Coil Air Pressure Drop	HVAC_PRESSURE		11	1
PARAM	c0465964-cfe0-4f19-81d7-80efaee10937	Chilled Water Connection 2 Diameter	PIPE_SIZE		1	1
PARAM	5c100465-61a3-42d7-82f6-d80709552d68	Ultraviolet Lights Number of Poles	NOOFPOLES		5	1
PARAM	8abbc665-508b-4b90-b37e-aade24369ec3	Condenser Fan Full Load Current	ELECTRICAL_CURRENT		10	1
PARAM	e0798666-b59d-4d08-8246-44451d113bbc	Heating Coil 4 Refrigerant Saturated Suction Temperature	HVAC_TEMPERATURE		6	1
PARAM	f41c6867-1c6e-4e4c-9a81-b67e72793de6	Exhaust Fan Power	ELECTRICAL_POWER		10	1
PARAM	ea976b67-3a71-41fc-9056-c5c19e47aee2	Return Fan Voltage	ELECTRICAL_POTENTIAL		5	1
PARAM	2dd5a867-86ee-438f-8f03-c4d83e849bed	Heating Coil Leaving Wet Bulb Temperature	HVAC_TEMPERATURE		6	1
PARAM	affeae67-368f-420d-9a15-d12cde583b81	Cooling Coil Actual Flow	PIPING_FLOW		6	1
PARAM	d1012068-2b06-46de-9f3a-9c1abeb95853	Cooling Coil Entering Wet Bulb Temperature	HVAC_TEMPERATURE		6	1
PARAM	8152a668-0af3-4760-9348-ea4c3f359635	Refrigerant Used	TEXT		8	1
PARAM	b0671c69-552f-4586-82be-a31092dc32c2	Glycol Type	TEXT		6	1
PARAM	e7826969-5392-43f1-9179-8810377b3d40	Cooling Coil Water Pressure Drop	PIPING_PRESSURE		6	1
PARAM	5a0c856a-2cd4-4def-80f5-fad804f54013	Heating Coil 2 Total Heating Capacity	HVAC_HEATING_LOAD		6	1
PARAM	fd1ff46a-46fa-4376-b850-1189fee956c8	Supply Fan Apparent Load	ELECTRICAL_APPARENT_POWER		10	1
PARAM	9141ad6b-bb04-4d71-b1e0-54b343cabdc3	Ultraviolet Lights 2 Apparent Load	ELECTRICAL_APPARENT_POWER		10	1
PARAM	1f58f26b-510f-408c-8901-425030a712e9	Enthalpy Wheel Apparent Load	ELECTRICAL_APPARENT_POWER		10	1
PARAM	2256056c-90f5-41b3-996d-b1726a7bbf21	Heating Coil 5 Sensible Heating Capacity	HVAC_HEATING_LOAD		6	1
PARAM	0eab1a6c-481d-4926-87d3-84790a9f45a0	Invalid Supply Air Flow	YESNO		11	1
PARAM	482b3c6c-fc88-4461-94a2-8f75c25f8c63	Waterside Economizer Cooling Coil Water Pressure Drop	PIPING_PRESSURE		6	1
PARAM	ccd8666c-bfbb-46cb-807c-b42413e62d5a	Ventilation Total Static Pressure	HVAC_PRESSURE		11	1
PARAM	8101dc6c-79b3-412f-ac9b-7b53ce57b34e	Condenser Diameter	LENGTH		1	1
PARAM	f81f266e-8d65-4fc3-87ab-c2c0ee50f8d8	Design Waterside Economizer Cooling Coil Water Flow	PIPING_FLOW		6	1
PARAM	86872b6e-2979-402b-98cf-a286578cea23	Simultaneous Cooling and Heating Efficiency	NUMBER		12	1
PARAM	0ff6716e-77b2-4207-9c99-cb6db8325678	Steam Output	NUMBER		6	1
PARAM	2fe7616f-d9ae-4e25-91f9-76db07a12b83	Return Fan HP	ELECTRICAL_POWER		10	1
PARAM	9328ba6f-2899-4e2a-8960-1de7a3c821d5	Design Cooling Air Flow Maximum	HVAC_AIR_FLOW		11	1
PARAM	cf827670-7a4c-4d5a-a651-79570bfb1f76	Exhaust Fan Quantity	INTEGER		6	1
PARAM	e9c27670-8d7d-4501-9afc-053727154677	Hood Intake Velocity	HVAC_VELOCITY		11	1
PARAM	70d88f70-a72d-4e36-8479-de23c77905ea	Filter 4 Efficiency	TEXT		11	1
PARAM	c0451071-aec8-4ece-a654-0c6d28e7a37c	Actual Oil Flow	PIPING_FLOW		6	1
PARAM	73bf5871-297a-410a-bbc3-a05fe20b44e8	Supply Fan Frequency	ELECTRICAL_FREQUENCY		6	1
PARAM	ac3e9d72-65db-4b62-a66a-828963156452	Supply Fan External Static Pressure	HVAC_PRESSURE		6	1
PARAM	ee99c872-31b3-4d63-ab6d-8b6bbfb88d6c	Supply Fan Blade Speed	NUMBER		6	1
PARAM	f4106573-4080-421e-836a-4803d87f0a3c	Heating Coil 4 Sensible Heating Capacity	HVAC_HEATING_LOAD		6	1
PARAM	478d7173-f09e-4899-aba7-6c8dbf672405	Supply Fan HP	ELECTRICAL_POWER		10	1
PARAM	5102b873-5fab-45b7-a2d0-f83ddee8d345	Product Name	TEXT		8	1
PARAM	36aa7b74-b8ac-4f6a-8a56-6115f35100cc	Unit Size	TEXT		1	1
PARAM	b1814775-9619-4b72-80e9-882e512cf476	Cooling Stages	INTEGER		14	1
PARAM	cd015375-e912-4a94-80fd-74b1c079d3a0	Primary Air Connection Height	HVAC_DUCT_SIZE		1	1
PARAM	90e26275-bc8f-42fc-85dc-319f988dbb6a	Cooling Coil Water Leaving Temperature	HVAC_TEMPERATURE		6	1
PARAM	4fb77f75-8018-4e65-8107-f11616763c77	Sound Attenuator Description	TEXT		6	1
PARAM	70dcae75-94be-4980-b62c-dc81bb14ff93	Evaporator Entering Temperature	PIPING_TEMPERATURE		6	1
PARAM	97c4bc76-05ab-4728-8017-830906ac4cb2	Heating Coil 5 Leaving Dry Bulb Temperature	HVAC_TEMPERATURE		6	1
PARAM	4cb51377-dc4d-4d9c-ba53-3856aff6ef64	Maximum Overcurrent Protection	ELECTRICAL_CURRENT		10	1
PARAM	f8ac2a77-2b17-4a6e-b631-457784c0f1fe	Kit Number	TEXT		8	1
PARAM	761aea77-6e27-4d27-97a8-aa1e16a420d2	Condenser Fan Phase	NOOFPOLES		5	1
PARAM	65b12278-b7e5-4553-b12b-bfc5139163c1	Condenser Fan Voltage	ELECTRICAL_POTENTIAL		5	1
PARAM	f81f2d78-184a-4e46-9705-57769b17fdb7	Filter 2 Efficiency	TEXT		11	1
PARAM	4ba76a78-2f46-48dd-8af4-6bb8e5af7084	Condenser Leaving Temperature for Cooling	PIPING_TEMPERATURE		6	1
PARAM	84189378-cfc6-4d21-83c6-95caaa3734c4	Waterside Economizer Cooling Coil Face Velocity	HVAC_VELOCITY		6	1
PARAM	a9a91679-d508-4baa-a5f7-e38020c4202f	Actual Air Flow	HVAC_AIR_FLOW		11	1
PARAM	d2343b79-3442-4f4b-b291-cac5ec56e14b	Heating Coil 3 Water Entering Temperature	HVAC_TEMPERATURE		6	1
PARAM	521d5d79-9948-46b9-86c4-344c86b188b5	Design Return Air Flow	HVAC_AIR_FLOW		11	1
PARAM	435d6179-dbf0-426a-a380-8eb617e01de4	Chilled Water Leaving Temperature	PIPING_TEMPERATURE		6	1
PARAM	4baa107a-51e8-4a5e-8528-f01f19eafd79	Cooling Coil 5 Leaving Wet Bulb Temperature	HVAC_TEMPERATURE		6	1
PARAM	e2cf747a-1b3d-4471-803a-9b33d7d0b56b	Supply Fan Description	TEXT		6	1
PARAM	5ce0e97a-a946-4650-8c51-7eb06b51bbbe	Return Fan Disconnect	TEXT		5	1
PARAM	c32aec7a-4daf-4615-aaf4-f0c7da196404	Condenser Coil Row Count	NUMBER		1	1
PARAM	aa53147b-f054-4efa-847f-cf9f057eb76b	Cooling Coil 3 Description	TEXT		6	1
PARAM	a270c77b-aa85-4d69-924a-0322df87f26f	Heating Coil 3 Entering Dry Bulb Temperature	HVAC_TEMPERATURE		6	1
PARAM	2bdfe47b-a1be-4768-834f-eb0f6dc952a7	Cooling Coil 4 Fin Density	NUMBER		6	1
PARAM	cac0907c-6c48-451c-b354-56b4641c1e96	Actual Heating Water Flow	PIPING_FLOW		6	1
PARAM	353f987c-5499-45c3-8ea4-04f509f5c5b9	Frequency	ELECTRICAL_FREQUENCY		5	1
PARAM	a181bf7c-4f8f-46f6-bb55-759896f21e22	Air Out Connection Diameter	HVAC_DUCT_SIZE		1	1
PARAM	6a65c57c-c305-4051-82e9-50c9677f6f2f	Cooling Coil 3 Water Leaving Temperature	HVAC_TEMPERATURE		6	1
PARAM	8412337d-5b32-471f-a5f3-e46f43deb555	Air Terminal Air Flow	HVAC_AIR_FLOW		11	1
PARAM	61f43a7d-d6f1-48ba-b946-e73214a86efe	Heating Coil Leaving Dry Bulb Temperature	HVAC_TEMPERATURE		6	1
PARAM	01b8147e-56a2-40c1-889d-243df798ae86	Heating Coil 3 Description	TEXT		6	1
PARAM	b2d37b7e-d535-421b-9664-5e4c0c452c3b	Ultraviolet Lights 2 Phase	NOOFPOLES		5	1
PARAM	9954967e-8184-432c-a7d9-f08b141f04c3	Sound Attenuator	YESNO		6	1
PARAM	89f0777f-4d43-4b29-8ae4-8b29e5712633	Design Supply Air Flow Minimum	HVAC_AIR_FLOW		11	1
PARAM	0abef57f-156d-4c53-bb19-ffa01df1864b	Filter Size	TEXT		11	1
PARAM	182a0880-9337-49f7-9ef9-3673505c4c47	Glycol Percentage	NUMBER		6	1
PARAM	071b3980-1c4a-493f-a27d-8751e96b30e7	Actual Fluid Cooler Water Flow	PIPING_FLOW		6	1
PARAM	ddeb4880-8d29-4d55-b376-4c4aff051b14	Supply Fan Type	TEXT		6	1
PARAM	78a75480-8cba-40a1-a85d-24f41e7ad16e	Total Static Pressure	HVAC_PRESSURE		14	1
PARAM	bb865f80-ebd5-4543-a511-249dfc43dadc	Cooling Coil 5 Water Entering Temperature	HVAC_TEMPERATURE		6	1
PARAM	0e0e6680-8e8a-496e-8d59-a6c867a1833d	Cooling Coil 4 Face Velocity	HVAC_VELOCITY		6	1
PARAM	6ac8ce80-f1f7-4ba4-92ef-a1e472f53e6d	High Temperature Heating Standard Rating Capacity	HVAC_HEATING_LOAD		14	1
PARAM	7437f280-2604-4220-81e2-9e77da6a7dc4	PreHeating Capacity	HVAC_HEATING_LOAD		14	1
PARAM	3c903b81-c72c-4574-a49e-06e8093f03cb	Stages of Capacity	INTEGER		6	1
PARAM	835a8081-7223-4485-b694-b588e77d1fba	Cooling Coil 4 Row Count	NUMBER		6	1
PARAM	4170ce81-c2c2-4530-81e6-a3a6266887a4	Altitude	LENGTH		6	1
PARAM	7b5d1182-c92f-4b2e-950a-0cf9c626c96e	Sound Rating	NUMBER		6	1
PARAM	3cfcd482-7f23-4449-9759-8d65ba8769b8	Heating Coil 2 Water Leaving Temperature	HVAC_TEMPERATURE		6	1
PARAM	63201983-5f4d-44f3-9fde-02ac4ffbd307	Exhaust Fan Phase	NOOFPOLES		5	1
PARAM	bbbe2983-5687-4f7a-b851-1857c68bfcb3	Exhaust Fan Type	TEXT		6	1
PARAM	47119d83-6eba-4ed1-937c-426f16eb4bfe	Cooling Coil 3 Water Pressure Drop	PIPING_PRESSURE		6	1
PARAM	ff0f7084-44dc-4869-8403-feac9518348b	Exhaust Fan Voltage	ELECTRICAL_POTENTIAL		5	1
PARAM	ee35ad84-b029-481a-b600-c9e17da63d7d	Material	TEXT		19	1
PARAM	bc961985-9ac6-4134-a5ba-11d1a3bba664	Cooling Coil 2 Face Velocity	HVAC_VELOCITY		6	1
PARAM	d3013185-f397-462b-995a-a363a3e1ecc0	Filter 3 Face Area	AREA		11	1
PARAM	69744185-563e-4b60-ad7d-552893e1c061	PreFilter Air Pressure Drop	HVAC_PRESSURE		11	1
PARAM	fadb2186-887d-40e9-badd-79fc879b5dfd	Cooling Coil 4 Actual Flow	PIPING_FLOW		6	1
PARAM	06b36486-aafc-4cde-ac5c-d54281e4bae8	Minimum Air Flow	HVAC_AIR_FLOW		11	1
PARAM	c96f8086-9714-4c50-972f-de52593ef63d	Heating Coil 2 Entering Dry Bulb Temperature	HVAC_TEMPERATURE		6	1
PARAM	e25eab86-c20e-474c-996a-ea5bb6745a05	Cooling Coil 4 Refrigerant Saturated Suction Temperature	HVAC_TEMPERATURE		6	1
PARAM	1ec3e686-13f7-4150-99bd-c88832d1fbdb	Cooling Coil Leaving Wet Bulb Temperature	HVAC_TEMPERATURE		6	1
PARAM	7c600087-15cb-4abb-bed5-9841adba3459	Supply Air Connection Diameter	HVAC_DUCT_SIZE		1	1
PARAM	60910087-6b86-4e3b-b137-bc404619d028	Heating Coil 4 Water Leaving Temperature	HVAC_TEMPERATURE		6	1
PARAM	929db387-33ff-45fc-af15-aa10763afb3b	Supply Air Connection Height	HVAC_DUCT_SIZE		1	1
PARAM	4910d787-840b-4e63-90de-0235847d1509	Notes	TEXT		8	1
PARAM	6e3edc87-68f2-414b-8837-f9c048cfa8de	Condenser Number of Passes	INTEGER		6	1
PARAM	a272e187-0271-4572-b3f4-b2783042b384	Filter 2 Quantity	NUMBER		11	1
PARAM	2cfaf887-8ec9-4aa2-85af-62413c884f95	Actual Supply Air Flow	HVAC_AIR_FLOW		11	1
PARAM	687c4188-e0c2-4a27-8f9b-9a161874f7fb	Filter 5 Efficiency	TEXT		11	1
PARAM	ae599f88-3734-46a0-9898-aa387c3cc71d	Condenser Coil Face Area	AREA		1	1
PARAM	aface988-0e12-4ab0-8640-8f82aad38ff8	Heat Pump Source Entering Temperature for Cooling	HVAC_TEMPERATURE		6	1
PARAM	0faa6e89-d984-4b95-8381-e2ab08165a62	Waterside Economizer Water Entering Temperature	PIPING_TEMPERATURE		6	1
PARAM	7f43e189-eb83-4cb1-aeec-620aff7d7795	Supply Fan Variable Frequency Drive	YESNO		6	1
PARAM	3d7a268a-5abb-4f16-9623-72ffa7d32a51	Condensate Drain Connection Diameter	PIPE_SIZE		1	1
PARAM	6af1528a-2809-43aa-b9a1-78e24b557b24	Electric Heat Phase	NOOFPOLES		5	1
PARAM	d437d58a-41c7-4637-9369-63f58f1163b1	Enthalpy Wheel Phase	NOOFPOLES		5	1
PARAM	612f068b-0e89-4dda-a656-0d961d27595d	Designation	TEXT		8	1
PARAM	dd00088b-392f-432d-bb0e-229f08d435a7	Latent Cooling Capacity 2	HVAC_COOLING_LOAD		14	1
PARAM	9c97098b-5ed6-4b7a-807a-d9b54558669b	Cooling Coil Glycol Percentage	NUMBER		6	1
PARAM	15b2198b-2177-491f-83ef-4e64d8d36156	Design Ventilation Air Flow	HVAC_AIR_FLOW		11	1
PARAM	106f2a8b-3006-4864-aaf0-d07ea744b6f1	Width	LENGTH		1	1
PARAM	0b77198c-a9f0-4a19-9a69-3214a60fd57d	Heat Pump Source Entering Temperature for Heating	HVAC_TEMPERATURE		6	1
PARAM	f3831d8c-b76a-4c2c-87fe-f659f1bd8328	Heating Stages	INTEGER		14	1
PARAM	70a6d08c-f384-428e-b950-1a741c86b400	Evaporator Pressure Drop	PIPING_PRESSURE		6	1
PARAM	92ec248d-2bbc-4bb4-87ee-583546f8fab8	Ultraviolet Lights 2 Number of Poles	NOOFPOLES		5	1
PARAM	ad8ba48d-c1b1-4787-8dde-e83adb21a3ad	Return Fan Frequency	ELECTRICAL_FREQUENCY		6	1
PARAM	bcdfc28d-5597-4f00-9713-91862e5f10fc	Condenser Fan Minimum Circuit Current	ELECTRICAL_CURRENT		10	1
PARAM	9cdfec8e-99b8-4bc3-89e8-adb230dc745a	Cooling Coil 4 Description	TEXT		6	1
PARAM	cea1ac8f-c231-47c5-ac6f-ad8db35aba9a	Compressor Full Load Current	ELECTRICAL_CURRENT		10	1
PARAM	71fc3e90-ab01-432f-8613-d905b0af5b95	Fluid Cooler Fan HP	ELECTRICAL_POWER		10	1
PARAM	2cae4190-06fd-40f2-8084-d93279403a75	Curb Width	LENGTH		1	1
PARAM	ff2a2892-eb5d-4f09-bf95-729d309c7996	Branch Connection Diameter	PIPE_SIZE		1	1
PARAM	e6d72293-7fbe-4792-adc5-561e74c62910	Average Annual Operating Cost	CURRENCY		12	1
PARAM	c495ef93-bebc-4334-ac19-733a0e9836b3	Supply Air Connection Quantity	INTEGER		11	1
PARAM	d5080994-c465-401b-999a-81f64d33b0ca	Cooling Coil 5 Air Pressure Drop	HVAC_PRESSURE		6	1
PARAM	2d482694-1287-40bd-917e-ef53c664aecb	Heating Coil Row Count	NUMBER		6	1
PARAM	9b29a194-9f72-42c5-8436-00d37ee41020	Apparent Load Circuit 2	ELECTRICAL_APPARENT_POWER		10	1
PARAM	472aaf94-e5c1-4747-87f7-8e7e11ceb698	Remote Evaporator	YESNO		6	1
PARAM	f666f494-5fdd-4fa6-a54c-8ca5f8c854bd	Waterside Economizer Cooling Coil Row Count	NUMBER		6	1
PARAM	3b75f894-0b45-4539-b948-4b5ac29d0d28	Compressor Phase	NOOFPOLES		5	1
PARAM	19215695-f34b-4f04-8e6a-676afaf8d7f9	Design Pump Water Flow	PIPING_FLOW		21	1
PARAM	d1f58b95-e5ea-4d8e-83da-44ead3237d92	Cooling Coil 4 Glycol Type	TEXT		6	1
PARAM	94f09195-9747-457a-9f5c-8de37687bb21	Heating Coil 4 Row Count	NUMBER		6	1
PARAM	34f8a795-517b-4daf-b4f6-009f6655b681	Cooling Coil 3 Leaving Wet Bulb Temperature	HVAC_TEMPERATURE		6	1
PARAM	2abcd395-4964-42f8-ac35-6f54b6b1f33a	Manifold Output 1 Diameter	PIPE_SIZE		1	1
PARAM	c55e8f96-70e3-4adc-82f0-2e81ec812b5b	Heating Coil 5 Actual Flow	PIPING_FLOW		6	1
PARAM	bd10cf96-8702-47f8-9ac8-cfdc4c6e784a	Cooling Coil 5 Glycol Percentage	NUMBER		6	1
PARAM	b8ed0897-3a22-4847-9edc-4d8c74b2fd38	Exhaust Fan Apparent Load	ELECTRICAL_APPARENT_POWER		10	1
PARAM	31100a97-af33-4e10-867a-972dbbdb5778	Heating Coil 3 Row Count	NUMBER		6	1
PARAM	9ce73797-048f-4b80-a1de-0d8c1cca66cc	Multizone Description	TEXT		6	1
PARAM	c5f25d97-91ad-48c8-96e2-99eac6fbb3f1	Product Page URL	URL		8	1
PARAM	59d56497-cbbf-45a7-9a2c-30039a7979a1	Design Chilled Water Flow	PIPING_FLOW		6	1
PARAM	03a08d97-66b1-4b89-87d2-b36ecaebb9be	High and Low Pressure Gas Equalizer Connection Diameter	PIPE_SIZE		1	1
PARAM	89beb397-51e9-4323-a6d9-a32a962dd6cf	Heating Coil 3 Leaving Wet Bulb Temperature	HVAC_TEMPERATURE		6	1
PARAM	0bc62698-80a5-435b-ae03-d2c9280e05e8	Cooling Coil 4 Air Pressure Drop	HVAC_PRESSURE		6	1
PARAM	54b94f98-ff17-457e-bc16-815012314fcc	Exhaust Fan Number of Poles	NOOFPOLES		5	1
PARAM	6ab9a598-d840-4d13-baa1-e3c04bd5d0ac	Supply Fan Drive	TEXT		6	1
PARAM	92f2a798-42f2-48fb-bfd2-e41a4e0059df	Actual Desuperheater Flow	PIPING_FLOW		6	1
PARAM	29f33699-a422-4d01-9b85-c8805b957300	Compressor 2 Minimum Circuit Current	ELECTRICAL_CURRENT		10	1
PARAM	db488499-4299-4a18-8678-f511db6b2b02	DX Coil Condensate Drain Connection Diameter	PIPE_SIZE		1	1
PARAM	8cf8f799-4f13-4bd8-8e74-5e8b9891964d	Actual Oil Cooler Water Flow	PIPING_FLOW		6	1
PARAM	d49c4c9a-b0a5-4a13-a2cc-b1a4580b55c6	Exhaust Total Static Pressure	HVAC_PRESSURE		11	1
PARAM	d0a2a99a-7bdf-4a15-abb8-16f5695a7380	Cooling Coil 2 Description	TEXT		6	1
PARAM	ca1cea9a-ef12-40d6-b2c6-f800376726e0	Compressor Type	TEXT		6	1
PARAM	7cb8149b-ab87-4a5e-9338-289c4e4a6e62	Air Terminal Velocity Pressure	HVAC_PRESSURE		11	1
PARAM	e862759b-7d8a-4c70-9863-791062221fcd	Heating Input	HVAC_HEATING_LOAD		14	1
PARAM	f9bf849b-1dda-4583-a7b7-56041558f49f	Chilled Water 2 Connection 2 Diameter	PIPE_SIZE		1	1
PARAM	f4e1d39b-76e5-43d5-b767-04ab67eceb8c	Air In Connection Width	HVAC_DUCT_SIZE		1	1
PARAM	6208849c-2d4a-4fd9-b5c1-77b0daec91ea	Cooling Coil 5 Actual Flow	PIPING_FLOW		6	1
PARAM	44dea79c-124b-4905-9de8-86b1e5fb4a41	Heating Coil Glycol Percentage	NUMBER		6	1
PARAM	bf6e0a9d-ed6a-4e65-a0d0-6c25cff01b00	High and Low Pressure Gas Connection Diameter	PIPE_SIZE		1	1
PARAM	c3bb1c9d-e334-46a7-b798-eaeaa3106f9b	Filter 2 Description	TEXT		11	1
PARAM	7fbc6c9d-def5-487e-a431-60b508de35ba	Heating Coil 3 Glycol Type	TEXT		6	1
PARAM	0b95a69d-9810-4cd3-9a75-4795fd245741	Blender Air Pressure Drop	HVAC_PRESSURE		11	1
PARAM	1eaae59d-f074-4611-b835-998bdf91c32d	Condenser Pressure Drop	PIPING_PRESSURE		6	1
PARAM	083e579e-5e19-45ec-af98-eb8d8349ce5a	Actual Variable Frequency Drive Water Flow	PIPING_FLOW		6	1
PARAM	5955729e-c2ff-4507-b823-fdc994790460	Heating Coil 5 Glycol Type	TEXT		6	1
PARAM	47d4729e-2c44-4294-a052-ed48123fff8e	Chilled Water 2 Entering Temperature	PIPING_TEMPERATURE		6	1
PARAM	9725f69e-600c-44d9-99c3-6938c1a0c3cc	Damper Pressure Drop	HVAC_PRESSURE		11	1
PARAM	75fd1a9f-3d4b-4eee-bc23-04fe2ed8c174	Design Exhaust Air Flow	HVAC_AIR_FLOW		11	1
PARAM	d5af03a0-1790-4976-94d2-fe6826287804	Steam Flow for Schedule	NUMBER		21	1
PARAM	8ddd76a0-f610-4ff0-8550-4b95d0c3e311	Refrigerant Liquid Connection Diameter	PIPE_SIZE		1	1
PARAM	8ca881a0-1ea3-4d67-83e2-832afcbb09bb	Electric Heat Control Steps	TEXT		6	1
PARAM	1ed1c3a0-60b5-44dc-b3cc-421d07bc9710	Cooling Coil Refrigerant Saturated Suction Temperature	HVAC_TEMPERATURE		6	1
PARAM	db2676a1-3605-4151-823f-2c999432e5af	Heating Coil 5 Row Count	NUMBER		6	1
PARAM	108cb6a1-7d8c-4c3d-9784-2f292e189386	Pump Head	PIPING_PRESSURE		6	1
PARAM	d82a02a2-6505-42cf-af1f-da72633d2700	Electric Heat Disconnect	TEXT		5	1
PARAM	e31c6ba2-44fa-4b0e-9a83-8668d291c254	Ultraviolet Lights Voltage	ELECTRICAL_POTENTIAL		5	1
PARAM	d44c94a2-9af6-4c51-af5a-d9e71a133044	Heating Coil 3 Face Velocity	HVAC_VELOCITY		6	1
PARAM	b25feca2-7ed4-418c-8036-7c70987f0753	Cooling Coil 4 Sensible Cooling Capacity	HVAC_COOLING_LOAD		6	1
PARAM	8bea60a3-65b5-46a0-a78f-af89cfc38af3	Return Fan Number of Poles	NOOFPOLES		5	1
PARAM	5f4788a3-d71b-41c4-9744-a34c75f218d1	Hood Throat Velocity	HVAC_VELOCITY		11	1
PARAM	dd0cefa3-e411-41e0-b0f0-5750511472e3	Cooling Coil 3 Glycol Percentage	NUMBER		6	1
PARAM	894818a4-429f-4f5b-a208-dd489db008fe	Exhaust Fan HP	ELECTRICAL_POWER		10	1
PARAM	cefa99a4-3d4d-4f87-9790-c11e8b694a3a	Manifold Input 2 Diameter	PIPE_SIZE		1	1
PARAM	4b2e80a5-e0de-463d-ac06-da0c48378d45	PreFilter Size	TEXT		11	1
PARAM	67fe81a5-825f-4bbd-bd9a-87ec6e552967	Exhaust Fan Variable Frequency Drive	YESNO		6	1
PARAM	5f4621a6-a54f-4583-9639-ba858ccbc19e	PreFilter Face Area	AREA		11	1
PARAM	72d65ea6-3136-4cf6-93e5-3061874a2753	Return Fan Apparent Load	ELECTRICAL_APPARENT_POWER		10	1
PARAM	334498a6-43e1-4ee8-8602-5dda9dde979d	Cooling Nominal Input Power	ELECTRICAL_POWER		10	1
PARAM	d18f27a7-967f-4f41-a0db-3ec3a9ac9bfb	Heating Coil 5 Water Pressure Drop	PIPING_PRESSURE		6	1
PARAM	07ea2fa7-2d52-4f94-898e-3b1eb3b02473	Filter 2 Width	LENGTH		1	1
PARAM	6e4ca3a7-4cf6-48d6-bbf2-f67fa1bd8b02	Ultraviolet Lights 2 Voltage	ELECTRICAL_POTENTIAL		5	1
PARAM	d804d2a7-58d1-4da4-9775-e84eeb510621	Condenser Entering Temperature for Cooling	PIPING_TEMPERATURE		6	1
PARAM	2c5eeaa7-7031-42c4-896b-ea58bba2572d	Return Fan Drive	TEXT		6	1
PARAM	be35f9a7-27e3-42b7-b9b4-18870ac02b84	Waterside Economizer Cooling Coil Face Area	AREA		6	1
PARAM	dc8c52a8-514e-405d-adbb-ab4a5f11b84f	PreHeating Coil Description	TEXT		6	1
PARAM	0fefb7a8-5886-4126-89a1-6770292b0445	Design Ventilation Air Flow Minimum	HVAC_AIR_FLOW		11	1
PARAM	5e53c8a8-e693-4f72-b0f9-459427271a71	Heating Coil 2 Water Entering Temperature	HVAC_TEMPERATURE		6	1
PARAM	3207ffa8-b9b9-44a0-a164-46b2581877bd	Cooling Coil Water Entering Temperature	HVAC_TEMPERATURE		6	1
PARAM	b88593a9-0cea-483c-8a7a-afb58bb3f979	Full Load Efficiency	NUMBER		12	1
PARAM	7c9193a9-caa6-47e3-8083-f7abccf7e615	Cooling Coil 5 Row Count	NUMBER		6	1
PARAM	2339b3a9-d6bd-439c-b3b4-eef10eb123d5	Steam In 2 Connection Diameter	PIPE_SIZE		1	1
PARAM	0763d9a9-2b80-4103-ac26-76c20a7d8ec3	Cooling Coil 5 Total Cooling Capacity	HVAC_COOLING_LOAD		6	1
PARAM	e779b2ab-13c2-44c0-bc7c-25d80095bf23	Manifold Input Diameter	PIPE_SIZE		1	1
PARAM	051f7dac-581c-4aca-a8f4-2fd3147be389	Filter 2 Air Pressure Drop	HVAC_PRESSURE		11	1
PARAM	f596bfac-a2be-460e-96ba-09d9c1aaa72f	Exhaust Fan Motor Speed	NUMBER		6	1
PARAM	d27342ad-12fa-4530-8650-bc8ce0c86f87	Cooling Coil 2 Sensible Cooling Capacity	HVAC_COOLING_LOAD		6	1
PARAM	4ddd66ad-1b99-4ade-b6bf-9a73dc34010a	PreFilter Efficiency	TEXT		11	1
PARAM	9ee299ad-d163-4335-82e2-9680512a469f	Steam Out 2 Connection Diameter	PIPE_SIZE		1	1
PARAM	2f7220ae-2cd8-4b61-a32a-451942a1c70c	Ventilation Air Connection Width	HVAC_DUCT_SIZE		1	1
PARAM	b0f461ae-941b-4d7f-a305-4fe42145cb68	Waterside Economizer Cooling Entering Dry Bulb Temperature	HVAC_TEMPERATURE		11	1
PARAM	407a74ae-eecd-45e1-bb21-77b6bc493367	Instantaneous Current Flow	ELECTRICAL_CURRENT		10	1
PARAM	31e69fae-3678-40aa-9682-24ed5e7b5195	Nominal Cooling Capacity 2	HVAC_COOLING_LOAD		14	1
PARAM	edfed9ae-a748-4e21-ac2a-95caef9339b1	Heating Coil 2 Description	TEXT		6	1
PARAM	4bb069af-e98d-4159-aaeb-dc3a434c0bc5	Installation Type	TEXT		20	1
PARAM	18618daf-4f3e-44fc-b075-58153baa3d6d	Cooling Coil 3 Refrigerant Saturated Suction Temperature	HVAC_TEMPERATURE		6	1
PARAM	acb411b0-dd6b-4fe6-bc02-8482e2a57f1e	Heating Water Connection Diameter	PIPE_SIZE		1	1
PARAM	93b857b0-f65a-4cba-9db9-98a23c2710dc	Heating Coil Water Pressure Drop	PIPING_PRESSURE		6	1
PARAM	5ebba0b0-a32b-41b6-9af7-72694128fd27	Actual Chilled Water 2 Flow	PIPING_FLOW		6	1
PARAM	40f9d3b0-a274-42a5-b990-80ae2aa13671	PreFilter Description	TEXT		11	1
PARAM	1d64eeb1-97b5-423c-8cbe-497d6d3cb989	Filter Face Area	AREA		11	1
PARAM	3e9656b2-3626-40ec-97c9-68b519a405ca	Air Terminal Static Pressure	HVAC_PRESSURE		11	1
PARAM	bef6a4b2-13a7-47ab-9e34-e63a756cf9a8	Cooling Coil 3 Entering Dry Bulb Temperature	HVAC_TEMPERATURE		6	1
PARAM	4c7537b3-91c4-4c79-868b-087793b7260e	Cooling Coil 2 Refrigerant Saturated Suction Temperature	HVAC_TEMPERATURE		6	1
PARAM	d8e738b3-1fdf-4b16-9ed7-c4ffc385104b	Cooling Coil 4 Leaving Wet Bulb Temperature	HVAC_TEMPERATURE		6	1
PARAM	28424bb3-165d-400d-857f-daa57a727186	Return Air Connection Diameter	HVAC_DUCT_SIZE		1	1
PARAM	055ba7b3-2217-4d84-8b1e-0b2e90fbc672	Exhaust Fan Locked Rotor Current	ELECTRICAL_CURRENT		10	1
PARAM	d3eccdb3-9937-4c42-9bbc-71ae697ccc05	Equipment Air Pressure Drop	HVAC_PRESSURE		11	1
PARAM	8e8e20b4-9311-4d18-98fd-764cd486e622	Header Connection Diameter	PIPE_SIZE		1	1
PARAM	0eb073b4-ccba-47b6-bd45-55baab2018c5	Exhaust Fan Minimum Circuit Current	ELECTRICAL_CURRENT		10	1
PARAM	ad07d0b4-3441-43ac-8f70-8936399f4ed3	Heating Coil 2 Glycol Type	TEXT		6	1
PARAM	0bba3eb5-f9eb-4fce-8460-2e8b6f5075d3	Number of Cells	INTEGER		6	1
PARAM	a55754b5-86da-49fe-b520-6983e572f696	Heating Coil 2 Sensible Heating Capacity	HVAC_HEATING_LOAD		6	1
PARAM	64cc6ab5-e9e5-44f5-a328-49a0319df1dc	Filter Quantity	NUMBER		6	1
PARAM	3f92abb6-db01-4c83-92ed-6de546af7004	Single Point Power Connection	YESNO		5	1
PARAM	5ff8b5b6-a719-4ba8-9574-dd5388eb82de	Heat Pump Coil Face Area	AREA		6	1
PARAM	ac9d21b7-2312-4c24-b85c-3864661641ed	Heating Coil 3 Total Heating Capacity	HVAC_HEATING_LOAD		6	1
PARAM	613046b7-4cb9-4984-9d46-51e263f6136a	Actual DX Coil Condensate Drain Flow	PIPING_FLOW		21	1
PARAM	b3f581b7-f7d1-4ad3-9c93-20a58720a171	Condenser Fan Power	ELECTRICAL_POWER		10	1
PARAM	3bb7a9b7-ebbf-4bfb-990d-5b7a1ed8db57	Throw Distance High Velocity	LENGTH		11	1
PARAM	e61041b8-1ae7-48de-9db6-65f2c51906aa	Integrated Energy Efficiency Ratio	NUMBER		12	1
PARAM	f41a71b8-c54b-49dd-8245-9327a406d97c	Heat of Rejection	HVAC_COOLING_LOAD		14	1
PARAM	ee1f8bb8-e503-49a8-bd5b-170d64400d82	Voltage	ELECTRICAL_POTENTIAL		5	1
PARAM	9446e3b9-cf4f-447f-8349-e62ed1be2122	Actual Return Air 2 Flow	HVAC_AIR_FLOW		11	1
PARAM	8c2655ba-30b9-487c-a520-d6d056fef1f4	Return Fan Motor Speed	NUMBER		6	1
PARAM	5fb684ba-8d67-4161-be61-6bf1d2dd446c	Equipment Served	TEXT		8	1
PARAM	1f9cbaba-0477-489e-a406-ee3dcf7a59ec	R Value	NUMBER		12	1
PARAM	bff8deba-b753-4bdf-922e-b20eb6e13666	Locked Rotor Current	ELECTRICAL_CURRENT		10	1
PARAM	e8a128bb-d75a-40f3-931d-591de2fab947	Relief Valve Connection Diameter	PIPE_SIZE		1	1
PARAM	a657e3bb-692c-44d5-a256-f23ad8f2c7a6	Curb Height	LENGTH		1	1
PARAM	685931bc-fdfb-4545-9df2-c34b24ca6e03	Cooling Coil Face and Bypass Air Pressure Drop	HVAC_PRESSURE		11	1
PARAM	94683fbc-f392-4424-a998-aa129ce4a6da	Filter Efficiency	TEXT		11	1
PARAM	1c1993bc-0271-4440-ac5c-51723d6c5439	Evaporator Number of Passes	INTEGER		6	1
PARAM	28bca3bc-5cd7-4970-a9c4-1d14ba73890a	Heating Coil 2 Leaving Dry Bulb Temperature	HVAC_TEMPERATURE		6	1
PARAM	3e8fb1bc-bdfc-4b6b-bba6-8eba09d396b0	Actual Heat Pump Condensate Drain Flow	PIPING_FLOW		21	1
PARAM	24ebc7bc-c0d1-473c-b41f-2cb407f1bd64	Cooling Coil 5 Refrigerant Saturated Suction Temperature	HVAC_TEMPERATURE		6	1
PARAM	cd8265bd-6b4d-433e-9016-2f589b2ee661	Exhaust Fan Blade Speed	NUMBER		6	1
PARAM	a8d593bd-ea95-499d-8943-7b11b64b129f	Blender Description	TEXT		6	1
PARAM	c1b618be-baef-4a77-8c0a-b485a353e20e	Evaporator Fouling Factor	NUMBER		6	1
PARAM	513ddfbe-b6fc-408f-a3c9-3ae2d0e2071e	Filter 2 Length	LENGTH		1	1
PARAM	3027fabe-96c5-4555-a12f-cb18b4e3ef4c	Curb Length	LENGTH		1	1
PARAM	f82302bf-0715-4423-8d40-a7893e9c4193	Oil Pressure Drop	PIPING_PRESSURE		6	1
PARAM	0bdf04bf-5d9d-4f79-b9d9-e8c361275daf	Air Terminal Total Pressure	HVAC_PRESSURE		11	1
PARAM	4de027bf-c4c2-4220-a7cc-55337537a245	Throw Distance Low Velocity	LENGTH		11	1
PARAM	a3bb9abf-c324-4a46-94de-e5d413c99640	Height	LENGTH		1	1
PARAM	92e3aebf-7130-421a-ae3f-9223934f98ad	Design Return Air Flow Minimum	HVAC_AIR_FLOW		11	1
PARAM	de163cc0-f0ec-4db4-841c-9e8d501a560e	Design Supply Air Flow	HVAC_AIR_FLOW		11	1
PARAM	09c365c0-4a7c-49b2-994b-f47be82a8971	Heating Coil 4 Total Heating Capacity	HVAC_HEATING_LOAD		6	1
PARAM	65f43fc1-c8f6-4d2e-8b4b-efcbcb7ce6e0	Filter 5 Size	TEXT		11	1
PARAM	94769bc1-9237-4b9a-87eb-b6bf6a6b0e9e	Latent Cooling Capacity	HVAC_COOLING_LOAD		14	1
PARAM	f5e9e3c1-8eda-4b36-945d-ddaf81e8473f	Cooling Coil Entering Dry Bulb Temperature	HVAC_TEMPERATURE		6	1
PARAM	a80af7c1-b148-4945-a017-ae0510faec3c	Heating Coil 2 Actual Flow	PIPING_FLOW		6	1
PARAM	e17b37c2-78b3-4702-8a53-a2308a6ede66	Design Heating Air Flow Minimum	HVAC_AIR_FLOW		11	1
PARAM	4217bac2-f608-4991-bcea-d83f48cf4138	Supply Fan Minimum Circuit Current	ELECTRICAL_CURRENT		10	1
PARAM	0fb442c5-a6c0-4903-87fb-b4d764c734d1	Condenser Leaving Temperature for Heating	PIPING_TEMPERATURE		6	1
PARAM	0e38ddc5-38f9-4ccd-a28c-84418ec9dedd	Heating Coil 4 Water Pressure Drop	PIPING_PRESSURE		6	1
PARAM	9a13fbc5-20e5-47a4-b803-a922e5c9ef26	Blender 2 Air Pressure Drop	HVAC_PRESSURE		11	1
PARAM	065f89c6-e350-4159-9aed-6820196ed201	Actual Valve Water Flow	PIPING_FLOW		21	1
PARAM	1a71e2c6-60a8-4bc1-bc69-8d6026d27e61	Heating Coil 3 Refrigerant Saturated Suction Temperature	HVAC_TEMPERATURE		6	1
PARAM	994541c8-ee54-44b2-bd6f-a83d99cd3bb1	Chilled Water Condensate Drain Connection Diameter	PIPE_SIZE		1	1
PARAM	ef74a7c8-997e-4bb8-80ab-edceb7fa352d	Electrical Disconnect	YESNO		5	1
PARAM	d3f7c6c9-ad59-4b3c-abb7-78f764f80362	EPA Rating	TEXT		8	1
PARAM	ad9ac8c9-791e-48a8-80bf-48d0def49af6	Heating Coil 3 Fin Density	NUMBER		6	1
PARAM	0e4bfcc9-7137-4f33-992a-e70cf17334af	Evaporator Relief Valve Connection Diameter	PIPE_SIZE		1	1
PARAM	7c4328ca-5fff-4f4e-b951-af0ee1c37d55	Exhaust Fan Drive	TEXT		6	1
PARAM	8ed442ca-c809-497c-93b3-c50b57115d3d	Refrigerant Charge	FORCE		6	1
PARAM	0e738bca-c404-402b-b3d4-7c7d4944efe6	Color	TEXT		19	1
PARAM	4a9420cb-4f59-4485-9dc7-ee6d66df732d	PreHeating Entering Wet Bulb Temperature	HVAC_TEMPERATURE		11	1
PARAM	220929cb-f982-45e3-97a4-80584c430545	Heating Coil Total Heating Capacity	HVAC_HEATING_LOAD		6	1
PARAM	cec2e9cb-9151-4b72-a3a6-2ebda7e2b2d4	Number of Poles	NOOFPOLES		5	1
PARAM	073304cc-9ffc-4b66-b6a6-8eb38a014edb	Cooling Coil 5 Water Leaving Temperature	HVAC_TEMPERATURE		6	1
PARAM	11b6a9cc-c9a2-4aba-86cd-d0601e07c827	Ventilation External Static Pressure	HVAC_PRESSURE		11	1
PARAM	faa2d1cc-9172-422f-8111-8950f9d98a83	Condenser Fan Number of Poles	NOOFPOLES		5	1
PARAM	bcc7dccc-a5e6-4a64-bba1-309bdbc94d46	Exhaust External Static Pressure	HVAC_PRESSURE		11	1
PARAM	8c3bfdcc-1411-4225-9f2e-84f8f208a2a6	Cooling Coil 2 Glycol Type	TEXT		6	1
PARAM	69fca9cd-53e6-469e-82e3-f5e2b4b40353	Waterside Economizer Cooling Coil Air Pressure Drop	HVAC_PRESSURE		11	1
PARAM	b73604ce-3cea-4230-b348-1986a7918fae	Supply Fan Motor Speed	NUMBER		6	1
PARAM	47fac8ce-7466-4f27-bc05-bdc46b4ea41b	Cooling Coil 2 Entering Wet Bulb Temperature	HVAC_TEMPERATURE		6	1
PARAM	024280cf-88a4-47a2-942b-13e417e49454	Filter 4 Face Area	AREA		11	1
PARAM	488898d0-44ad-4298-b50b-5f52646f794d	Cooling Coil 3 Fin Density	NUMBER		6	1
PARAM	603de3d0-3414-4e30-848f-ea2a80701483	Cooling Coil Leaving Dry Bulb Temperature	HVAC_TEMPERATURE		6	1
PARAM	f7e315d1-a564-4b36-a758-a4d9234ec4c5	Heating Coil 4 Leaving Dry Bulb Temperature	HVAC_TEMPERATURE		6	1
PARAM	dd673ad1-9437-4e1b-81a6-22b9d2d272a7	Steam Out Connection Diameter	PIPE_SIZE		1	1
PARAM	98c07fd1-1f98-4016-b30e-dff8732fe9b4	Compressor Stages	TEXT		14	1
PARAM	a2fbbfd1-51ea-4a25-828c-af81885fa710	Heating Coil 5 Entering Dry Bulb Temperature	HVAC_TEMPERATURE		6	1
PARAM	ee98d0d1-ed87-46ff-9dd3-e93dd3ff6789	Nominal Part Load Value	NUMBER		12	1
PARAM	9cf1e9d1-ba10-4d28-86ee-59e0a25a6ab2	Design Ambient Summer Dry Bulb Temperature	HVAC_TEMPERATURE		12	1
PARAM	2fc83dd2-9aca-4fdc-85e3-338818e1aa04	Minimum Percent Air Flow	NUMBER		11	1
PARAM	4dccecd3-d48e-4c7a-bba2-03dfa4e9668d	Actual Air Flow Imbalance	HVAC_AIR_FLOW		11	1
PARAM	163a2cd4-c83f-4559-8130-838e1f024258	Actual Evaporator Flow	PIPING_FLOW		6	1
PARAM	e24369d4-3bcd-43d2-bde9-ec932803693a	Actual Vertical Refrigerant Pipe Length Below Unit	LENGTH		6	1
PARAM	e3bc86d4-a43e-4dde-a4cb-476dfa34a1cf	Shipping Weight	FORCE		8	1
PARAM	0d7b36d5-683a-43f9-b30e-484f275f4888	Actual Supply Air Connection 4 Flow	HVAC_AIR_FLOW		11	1
PARAM	07f96fd5-f741-4436-910e-4158e174bf4f	PreHeating Water Entering Temperature	PIPING_TEMPERATURE		6	1
PARAM	05d05bd6-ae35-4b80-95e9-b5b24ac47103	Filter Face Velocity	HVAC_VELOCITY		6	1
PARAM	b87281d6-5696-40cf-afbe-35ff51db335f	Primary Air Connection Diameter	HVAC_DUCT_SIZE		1	1
PARAM	9131a4d6-b41c-4164-b228-b05186f54fab	Condenser Entering Temperature for Heating	PIPING_TEMPERATURE		6	1
PARAM	3003c9d6-f1dd-4171-86c3-f8914246117e	Curb Exists	YESNO		20	1
PARAM	b3464bd7-b0ec-4345-a4bc-0a805cd77fd1	Heating Coil 2 Row Count	NUMBER		6	1
PARAM	dc41e7d7-c860-4fed-ab0a-d9aef1c59ffa	Ventilation Air Connection Diameter	HVAC_DUCT_SIZE		1	1
PARAM	5df563d8-778d-44d2-b0f3-058ccfe732fc	Filter Description	TEXT		11	1
PARAM	e226a9d8-1a8b-4ed7-986a-567e39a559c7	Water Connection Diameter	PIPE_SIZE		1	1
PARAM	221aefd8-9bcf-4b11-8483-294328440013	PreHeating Coil Face and Bypass Air Pressure Drop	HVAC_PRESSURE		11	1
PARAM	385f6cda-3461-4827-bd85-8c4cc494366d	Seasonal Energy Efficiency Rating	NUMBER		12	1
PARAM	a6f784da-c960-4cc3-afdb-a4dba48eb0a8	Waterside Economizer Cooling Coil Fin Density per Inch	NUMBER		6	1
PARAM	508894da-f67a-449a-8133-ae73395ae7ac	Filter 2 Face Velocity	HVAC_VELOCITY		6	1
PARAM	261ed6da-7043-4241-ba2c-fbd1ca0053d7	Heat of Absorption	HVAC_HEATING_LOAD		14	1
PARAM	298915db-d1af-4f5a-acc3-a276d09f2287	Condenser Fan Apparent Load	ELECTRICAL_APPARENT_POWER		10	1
PARAM	0e539bdb-5a35-4573-98cc-324c793721bd	Heating Coil Face Velocity	HVAC_VELOCITY		6	1
PARAM	2d4afbdb-2d08-4d25-beaa-1c756e9d87af	Length of Interconnecting Refrigerant Pipe	LENGTH		6	1
PARAM	11671fdc-1685-42ae-aa2e-c189cd754176	Enthalpy Wheel Voltage	ELECTRICAL_POTENTIAL		5	1
PARAM	510d32dc-a211-4f0b-a089-02b5ad9fadc4	Control Description	TEXT		8	1
PARAM	16b79adc-1021-413e-ac7a-3ab465c150d8	Cooling Coil 3 Entering Wet Bulb Temperature	HVAC_TEMPERATURE		6	1
PARAM	878768dd-1593-413b-b748-0a0683fd0c9d	Economizer Description	TEXT		6	1
PARAM	1575bcdd-e076-4575-aa72-b1044e73d3da	Humidifier Description	TEXT		6	1
PARAM	0f308dde-801a-451a-a99e-e1490589b7d1	Heating Coil 5 Description	TEXT		6	1
PARAM	678199de-3bca-4c40-9375-1e5e35e8171f	High Temperature Coefficient of Performance	NUMBER		12	1
PARAM	137ca1de-d1f7-4f40-a33c-cd1ce096710d	Waterside Economizer Cooling Leaving Dry Bulb Temperature	HVAC_TEMPERATURE		11	1
PARAM	c319a9de-c921-4c80-ae38-7b0f3e496aa1	Pressure Rating	HVAC_PRESSURE		6	1
PARAM	3a46f2de-0b6e-47e2-b389-0322365fb5c4	Heating Coil 3 Glycol Percentage	NUMBER		6	1
PARAM	0e4028df-7a13-4649-811c-901a5c88e63d	System Served	TEXT		8	1
PARAM	fcf72edf-9ad5-4dd7-b3ba-7441b013512a	Air In Connection Diameter	HVAC_DUCT_SIZE		1	1
PARAM	2c2894df-c283-4a8a-a041-b556c5047a55	Apparent Load Circuit 3	ELECTRICAL_APPARENT_POWER		10	1
PARAM	03b0b2df-3217-4c3a-ad74-d3aedae10e2f	Return Fan Variable Frequency Drive	YESNO		6	1
PARAM	d162c2df-3490-42ca-ae67-99e1fc657ffe	Heating Coil 5 Water Entering Temperature	HVAC_TEMPERATURE		6	1
PARAM	ff0990e0-f4fd-4f87-8919-7383edb4b24a	Return Fan Blade Speed	NUMBER		6	1
PARAM	d92dbae0-347d-4e8e-a815-a77ea44f38ff	Supply Fan Disconnect	TEXT		5	1
PARAM	f695fde0-3f94-4530-abf9-7fd0e5e88457	Length	LENGTH		1	1
PARAM	7d3d19e1-9d59-4529-9208-9876d6a9797b	Heating Coil 4 Air Pressure Drop	HVAC_PRESSURE		6	1
PARAM	e1b291e1-80ba-45c9-9da8-dc83f36a0c17	Evaporator Water Connection Diameter	PIPE_SIZE		1	1
PARAM	e12c99e1-d3f4-45e2-9b46-e40af3d78241	Cooling Coil 5 Glycol Type	TEXT		6	1
PARAM	50ea53e2-1696-45fe-8377-b78101915bfe	Steam In Connection Diameter	PIPE_SIZE		1	1
PARAM	147865e2-5329-438a-b37f-3affebc5937f	Pump Full Load Current	ELECTRICAL_CURRENT		10	1
PARAM	37956de2-c78c-419d-bdfa-96de64244eb3	Refrigerant Saturated Suction Temperature	HVAC_TEMPERATURE		6	1
PARAM	9e15efe2-aeac-40fa-9d06-65b58139fc76	Chilled Water Connection Diameter	PIPE_SIZE		1	1
PARAM	3a4909e3-6a82-4998-b395-3ada9a99bca6	Air Out Connection Width	HVAC_DUCT_SIZE		1	1
PARAM	78ce7ce3-aba8-4570-a7d7-038e46cd3b71	Actual Ventilation Air Flow	HVAC_AIR_FLOW		11	1
PARAM	d74789e3-4182-46e2-bf17-40c216087c34	Sound Discharge Noise Criteria	NUMBER		6	1
PARAM	894284e4-ba70-4b89-8725-467fd975c041	Filter Width	LENGTH		1	1
PARAM	f581cae4-9d13-456b-a180-fca24d87b9c6	Tank Type	TEXT		21	1
PARAM	c1b568e5-747d-409a-a738-81e09c81e60e	Heating Coil 2 Face Velocity	HVAC_VELOCITY		6	1
PARAM	2aef75e5-a454-4e57-9c20-03d15aed2d0a	Cooling Coil Face Velocity	HVAC_VELOCITY		6	1
PARAM	c29d7ee5-c867-4c29-9edc-f946e5a00f59	Gas Heat Input Power	HVAC_HEATING_LOAD		14	1
PARAM	75d296e5-aa22-4bd7-bcc8-9d5151542981	Cooling Coil 2 Glycol Percentage	NUMBER		6	1
PARAM	3e6ad9e5-be7e-462f-9535-07554ba3e95d	Filter 2 Size	TEXT		11	1
PARAM	934bebe5-4d32-4c82-9fba-9b3000ebabc7	Cooling Coil Glycol Type	TEXT		6	1
PARAM	d4a31de6-42af-40eb-bef3-331be3b924cd	Cooling Coil 2 Leaving Dry Bulb Temperature	HVAC_TEMPERATURE		6	1
PARAM	a09335e6-e752-425c-ba68-3e8235f530c2	Integrated Part Load Value	NUMBER		12	1
PARAM	df2279e7-23e4-4876-a7f2-a6aa5f2c2b19	Valve Pressure Drop	PIPING_PRESSURE		6	1
PARAM	d33ffde7-99c3-4572-9cfa-caab1ee42020	Heating Coil 5 Fin Density	NUMBER		6	1
PARAM	2fc51ee8-7829-4250-8809-6fc0472bd7f7	Heating Water Connection 2 Diameter	PIPE_SIZE		1	1
PARAM	ab55ace8-dd66-4303-86e6-b34c44baa784	Cooling Coil 3 Leaving Dry Bulb Temperature	HVAC_TEMPERATURE		6	1
PARAM	8cf2aee8-c1f8-498b-9faa-76722435e771	Filter Air Pressure Drop	HVAC_PRESSURE		11	1
PARAM	645ae6e8-f7ee-4e69-bab7-44581d144da8	Air Leakage	NUMBER		12	1
PARAM	c6b0f8e8-3ae1-489d-9c15-9bcfe3a7c976	PreHeating Coil Face and Bypass Description	TEXT		6	1
PARAM	19bd8ce9-d351-4fc3-a341-28586db97722	Low Temperature Coefficient of Performance	NUMBER		12	1
PARAM	3f8696e9-2b5a-4a6a-b095-013bd4bf9a3f	Enthalpy Wheel Air Pressure Drop	HVAC_PRESSURE		11	1
PARAM	9c3507ea-7349-4ffc-a218-dba43b5f9ce2	Compressor 2 Full Load Current	ELECTRICAL_CURRENT		10	1
PARAM	4d2d47ea-739a-4c50-809d-67499795a08a	Steam Connection Diameter	PIPE_SIZE		1	1
PARAM	f6b3a3ea-3d2d-4553-bd02-3ce7ddd7ad81	Exhaust Air Connection Width	HVAC_DUCT_SIZE		1	1
PARAM	a66ce4ea-9966-4361-85e3-61c5f8d34071	Boiler Water Pressure Drop	PIPING_PRESSURE		6	1
PARAM	0dab0ceb-7473-4507-8a2a-e9b5aaea43e9	Desuperheater Water Connection Diameter	PIPE_SIZE		1	1
PARAM	b5e71aeb-1293-4b3e-928e-d50e682466b9	Parts Catalog URL	URL		8	1
PARAM	328971eb-c691-4921-bea9-abd0308db9aa	Condenser Fouling Factor	NUMBER		6	1
PARAM	74c7d8eb-def1-4ad6-bf7c-97012c37b784	Cooling Coil 3 Total Cooling Capacity	HVAC_COOLING_LOAD		6	1
PARAM	ddf17cec-53a6-4a07-b8ea-4629bccac097	Heating Coil 4 Leaving Wet Bulb Temperature	HVAC_TEMPERATURE		6	1
PARAM	971e8fec-20f3-4af4-875d-e3314d10860c	Heating Coil Actual Flow	PIPING_FLOW		6	1
PARAM	a38498ed-94b5-46a6-9074-a154ac5d9fa0	Cooling Coil 3 Row Count	NUMBER		6	1
PARAM	d12fcced-022c-4485-b720-993aabd659e8	Oil Cooler Water Pressure Drop	PIPING_PRESSURE		6	1
PARAM	b90b3cee-e2c7-46c7-a89d-50fa13cd7373	Design Primary Air Flow Maximum	HVAC_AIR_FLOW		11	1
PARAM	2004efee-9c4b-45ed-aef0-57c7853cea97	Compressor Power	ELECTRICAL_POWER		10	1
PARAM	f850f9ee-b3e1-4373-aed6-b37eda1751ef	Water Treatment Pressure Drop	PIPING_PRESSURE		6	1
PARAM	299415ef-698d-4643-aa6d-b52f0627bf7c	Variable Frequency Drive Water Pressure Drop	PIPING_PRESSURE		6	1
PARAM	39ce85ef-c66b-41c5-92ad-3d5f27f63872	Cooling Coil 5 Description	TEXT		6	1
PARAM	c116acef-6cc2-4737-9fdb-8aa0af3cfc50	Actual Condenser Flow	PIPING_FLOW		6	1
PARAM	9767caef-2a2a-4744-b7fd-bafc09b113f0	Design Valve Water Flow	PIPING_FLOW		21	1
PARAM	4e9eedef-bd42-4003-a995-b98a14622fb9	Heating Coil 4 Glycol Percentage	NUMBER		6	1
PARAM	f27156f0-6144-4293-b8a1-17f0dbffd0b5	Design Ventilation Air Flow Maximum	HVAC_AIR_FLOW		11	1
PARAM	c1af76f0-86ad-4755-a0fc-4e2148609531	PreFilter Depth	LENGTH		1	1
PARAM	7dbbaff0-b55a-4f33-8fd4-9dc33f59a280	Condenser Leaving Temperature	PIPING_TEMPERATURE		6	1
PARAM	d7f2c1f0-f3d3-4d8f-a898-035d75e2f6f0	Evaporator Coil Temperature	HVAC_TEMPERATURE		6	1
PARAM	f598e4f0-f835-4aca-9ecd-ce1160cb384e	Condenser Entering Temperature	PIPING_TEMPERATURE		6	1
PARAM	ab2439f1-b99c-4918-bdca-772118ce2459	Filter 5 Description	TEXT		11	1
PARAM	c1a39df1-5152-46c4-8c90-25f66750a60c	Heating Coil 4 Face Velocity	HVAC_VELOCITY		6	1
PARAM	ee4aecf1-c02b-4852-be3c-4cc4d1001743	Filter 3 Size	TEXT		11	1
PARAM	b9a6b5f2-1be8-465f-9046-648da0d48c01	Economizer Type	TEXT		6	1
PARAM	ea7ce6f2-4c26-4672-b695-b004b46a68dd	Condenser Fan Variable Frequency Drive	YESNO		6	1
PARAM	84a0a0f3-6615-4d1e-b675-0d9fd7ce6336	Maximum Vertical Refrigerant Pipe Length Below Unit	LENGTH		6	1
PARAM	c298acf3-7e82-481c-9f43-bc48c40d8a01	Heating Coil 5 Air Pressure Drop	HVAC_PRESSURE		6	1
PARAM	bddc75f4-8e27-4afc-add0-de7358bbf6d3	Product Documentation Link	URL		8	1
PARAM	f01d6af5-a0ea-48d5-9f65-08a640226fbd	Maximum Overcurrent Device Type	TEXT		10	1
PARAM	21c594f5-ffa6-4744-a300-989626a13672	Cooling Coil Air Pressure Drop	HVAC_PRESSURE		6	1
PARAM	f1adccf5-acbd-4e0b-b15c-8bcbbc4aab16	PreHeating Water Leaving Temperature	PIPING_TEMPERATURE		6	1
PARAM	87591bf6-2c0d-4bd0-aafc-b4415e94f18b	Blender 2 Description	TEXT		6	1
PARAM	0445c9f6-1c34-4101-8065-4ed980320790	Cooling Coil 5 Face Velocity	HVAC_VELOCITY		6	1
PARAM	80a319f7-7756-4dbe-bc70-be2158171bc3	Cooling Coil 4 Entering Wet Bulb Temperature	HVAC_TEMPERATURE		6	1
PARAM	6ee196f7-9df0-49a1-943c-5475f26ed378	Heating Coil 5 Leaving Wet Bulb Temperature	HVAC_TEMPERATURE		6	1
PARAM	40b11ef8-547f-417e-bee4-3ec1ce1f240b	PreHeating Leaving Dry Bulb Temperature	HVAC_TEMPERATURE		11	1
PARAM	6e8526f8-eb62-4103-90a9-41772855048f	Electric Heat Number of Poles	NOOFPOLES		5	1
PARAM	7b2c43f8-f816-49fb-9796-2e126752a9ee	Cooling Coil 2 Actual Flow	PIPING_FLOW		6	1
PARAM	47439af8-c7fe-45ef-9341-eaab85594311	Return Total Static Pressure	HVAC_PRESSURE		11	1
PARAM	97e02bf9-0e22-41da-854f-cff85dd8b099	Full Load Current	ELECTRICAL_CURRENT		10	1
PARAM	80c1f5f9-ef6a-46b8-8b2c-aab2298c007e	Heating Coil 3 Leaving Dry Bulb Temperature	HVAC_TEMPERATURE		6	1
PARAM	8e7733fa-561e-4264-8948-3005268b32b5	Cooling Coil 2 Water Pressure Drop	PIPING_PRESSURE		6	1
PARAM	4c02a9fa-1adb-42d2-9c33-bf37871bd94d	Design Fan Powered Box Primary Air Flow	HVAC_AIR_FLOW		11	1
PARAM	b50f1ffb-6b71-4022-9c3b-7fa0a553ceb1	Cooling Coil 3 Sensible Cooling Capacity	HVAC_COOLING_LOAD		6	1
PARAM	857732fb-7721-4d42-9d8c-6ab16ccae883	Supply Fan Power	ELECTRICAL_POWER		10	1
PARAM	697795fb-88ee-4cc9-93e4-e363ae8be74b	Phase	NOOFPOLES		5	1
PARAM	0bff9dfb-9268-49eb-b3d5-b87644efc25c	Operating Mode	TEXT		8	1
PARAM	e40bd7fb-0f08-4c40-935b-d2047ad78b31	Sump Heater Power	ELECTRICAL_POWER		10	1
PARAM	844826fc-e1b9-4f9f-8563-09086f90f547	Location	TEXT		8	1
PARAM	f6eb65fc-3548-4622-8cbf-423c32d7b2f4	Supply External Static Pressure	HVAC_PRESSURE		11	1
PARAM	517b94fc-ff9a-46a4-aec1-65529b74103a	Electric Heat Minimum Circuit Current	ELECTRICAL_CURRENT		10	1
PARAM	b044dbfc-4798-4622-8776-5256ae49de43	Refrigerant Liquid Connection 2 Diameter	PIPE_SIZE		1	1
PARAM	377c22fd-2bc2-4fc8-a438-08242f815920	Actual Supply Air Connection 2 Flow	HVAC_AIR_FLOW		11	1
PARAM	b7ab36fd-20eb-4514-bca4-9c000854ac52	Cooling Coil 5 Water Pressure Drop	PIPING_PRESSURE		6	1
PARAM	1ae553fd-a006-4d5d-a240-5e15e39083ce	PreHeating Coil Face Velocity	HVAC_VELOCITY		6	1
PARAM	90cf7efd-4a2f-4438-be99-640dd202ab99	Cooling Coil 2 Water Leaving Temperature	HVAC_TEMPERATURE		6	1
PARAM	2a91b0fd-1d30-4460-a431-a7a28aa69007	Energy Star Zone	TEXT		23	1
PARAM	6461c8fd-4107-4339-8848-4f19b33863c8	Heating Coil 3 Sensible Heating Capacity	HVAC_HEATING_LOAD		6	1
PARAM	6aa52afe-b294-4f4f-ade0-fe45695e3f9a	Design Evaporator Flow	PIPING_FLOW		6	1
PARAM	50d352fe-e78b-4792-9472-be27e7305e58	Heating Coil 3 Actual Flow	PIPING_FLOW		6	1
PARAM	54eabdfe-5d27-46c6-9a91-9e1fbb8f602d	Heating Coil Glycol Type	TEXT		6	1
PARAM	e00288ff-4682-4d38-bdb3-86149700c21c	Invalid Heating Leaving Dry Bulb Temperature	YESNO		11	1
