 ,Model##Other##,Length##Length##Inches,Width##Length##Inches,Height##Length##Inches,Refrigerant Used##Other##,Evaporator Water Connection Diameter##pipe_size##inches,Water Connection Between Connections##Length##Inches,Water Connection Offset Bottom##Length##Inches,Refrigerant Liquid Connection Diameter##pipe_size##inches,Liquid Connection Offset Bottom##Length##Inches,Liquid Connection Between Connections##Length##Inches,Water Connections Protrusion##Length##Inches,Refrigerant Suction Gas Connection Diameter##pipe_size##inches,Suction Gas Connection Offset Top##Length##Inches,Suction Gas Connection Between Connections##Length##Inches,Refrigerant Connections Protrusion##Length##Inches,Clearance Offset Top##Length##Inches,Clearance Offset Right##Length##Inches,Clearance Offset Left##Length##Inches,Clearance Offset Front##Length##Inches,Clearance Offset Bottom##Length##Inches,Clearance Offset Back##Length##Inches,Family Load Status##other##,Include Clearance##Other##
"30 Ton, for AGZ030EB",AGZ030EB,7.27,9.84,21.18,R-410A,2.5,14.53,4.27,0.875,3.55,6.54,1.89,1.625,1.87,6.1,1.18,12,12,12,12,0,12,Valid – Type loaded via type catalog,1
"35 Ton, for AGZ035EB",AGZ035EB,7.96,9.84,21.18,R-410A,2.5,14.53,4.27,0.875,3.55,6.54,1.89,1.625,1.87,6.1,1.18,12,12,12,12,0,12,Valid – Type loaded via type catalog,1
"40 Ton, for AGZ040EB",AGZ040EB,8.65,9.84,21.18,R-410A,2.5,14.53,4.27,0.875,3.55,6.54,1.89,1.625,1.87,6.1,1.18,12,12,12,12,0,12,Valid – Type loaded via type catalog,1
"45 Ton, for AGZ045EB",AGZ045EB,10.04,9.84,21.18,R-410A,2.5,14.53,4.27,1.125,3.55,6.54,1.89,1.625,1.87,6.1,1.18,12,12,12,12,0,12,Valid – Type loaded via type catalog,1
"50 Ton, for AGZ050EB",AGZ050EB,11.43,9.84,21.18,R-410A,2.5,14.53,4.27,1.125,3.55,6.54,1.89,1.625,1.87,6.1,1.18,12,12,12,12,0,12,Valid – Type loaded via type catalog,1
"55 Ton, for AGZ055EB",AGZ055EB,12.12,9.84,21.18,R-410A,2.5,14.53,4.27,1.125,3.55,6.54,1.89,1.625,1.87,6.1,1.18,12,12,12,12,0,12,Valid – Type loaded via type catalog,1
"60 Ton, for AGZ060EB",AGZ060EB,7.66,12.68,31.13,R-410A,3,22.36,5.4,1.375,3.95,8.82,2.04,2.125,2.3,8.07,2.05,12,12,12,12,0,12,Valid – Type loaded via type catalog,1
"65 Ton, for AGZ065EB",AGZ065EB,8.9,12.68,31.13,R-410A,3,22.36,5.4,1.375,3.95,8.82,2.04,2.125,2.3,8.07,2.05,12,12,12,12,0,12,Valid – Type loaded via type catalog,1
"70 Ton, for AGZ070EB",AGZ070EB,8.9,12.68,31.13,R-410A,3,22.36,5.4,1.375,3.95,8.82,2.04,2.125,2.3,8.07,2.05,12,12,12,12,0,12,Valid – Type loaded via type catalog,1
