
ALWAYS GET THE LATEST VERSION OF REVIT CONTENT BEFORE USING THEM IN A PROJECT.


Family File Dates: 2013 October 1
  - Rebranded to Daikin Applied


Family File Dates:  2011 September 2
  - Added the new "Condensing Section Height" parameter to support the differences in geometry for new sizes available



Family File Dates:  2010 December 16
  - Added the new "Parts Catalog URL" parameter to the new online parts catalog (http://www.mcquay.com/McQuay/BIM/PartsCatalog)
  - Fan grill circles were accidentally set to be hidden lines.  Changed to solid lines.
  - Added missing Exhaust Fan parameters
  - Improved the constraints for the main box extrusion and duct connectors



Family File Dates:  2010 October 29
  - Reduced nested family usage and simplified geometry to decrease the file sizes and impact to Revit's performance
  - Removed steam flow parameters until Revit supports Mass/Time units of measure



Family File Dates: 2010 May 21

  - Upgraded to Revit 2010 format.  Changes include:
    - OmniClass value added
    - Clearance volume changed to green (easier to see in Revit interference checks)
    - Set materials "Render Appearance" settings to create better images when the model is rendered
    - “Product Page URL” parameter added for conformance to the Revit Model Content Style Guide
    - "URL" parameter value conforms better to Revit Model Content Style Guide 
    - To reduce load on Revit, web link parameters were changed to Type parameters
    - To improve usage for system design purposes, parameters such as those for capacities, temperatures, power values and others were changed to Instance parameters

