 ,Model##Other##,Length##Length##Inches,Width##Length##Inches,Height##Length##Inches,Compressor Type##Other##,Refrigerant Used##Other##,Compressor Quantity##Other##,Evaporator Offset Front##Length##Inches,Evaporator Offset Bottom##Length##Inches,Evaporator Height##Length##Inches,Evaporator Offset Left##Length##Inches,Connections Offset Left##Length##Inches,Suction 1 Offset Front##Length##Inches,Suction 1 Offset Bottom##Length##Inches,Suction 2 Offset Front##Length##Inches,Refrigerant Suction Gas Diameter##pipe_size##inches,Refrigerant Liquid 2 Connection Offset Front##Length##Inches,Refrigerant Liquid Connection Offset Front##Length##Inches,Refrigerant Liquid Connection Offset Bottom##Length##Inches,Refrigerant Liquid Connection Diameter##pipe_size##inches,Hot Gas Offset Bottom##Length##Inches,Hot Gas Connection Diameter##pipe_size##inches,Base Rail Width##Length##Inches,Clearance Offset Top##Length##Inches,Clearance Offset Right##Length##Inches,Clearance Offset Left##Length##Inches,Clearance Offset Front##Length##Inches,Clearance Offset Bottom##Length##Inches,Clearance Offset Back##Length##Inches,Family Load Status##other##,Include Clearance##Other##
140 Ton,AGZ140E,237.2,88,92.7,SCROLL,R-410A,4,24,6,30,150,133.5,40,34.7,8,2.63,7.4,32.6,8.9,1.13,6.8,1.13,4,150,48,48,48,0,96,Valid – Type loaded via type catalog,1
150 Ton,AGZ150E,237.2,88,92.7,SCROLL,R-410A,4,24,6,30,150,133.5,40,34.7,8,2.63,7.4,32.6,8.9,1.13,6.8,1.13,4,150,48,48,48,0,96,Valid – Type loaded via type catalog,1
161 Ton,AGZ161E,237.2,88,92.7,SCROLL,R-410A,4,24,6,30,150,133.5,40,34.7,8,2.63,7.4,32.6,8.9,1.13,6.8,1.13,4,150,48,48,48,0,96,Valid – Type loaded via type catalog,1
