 ,Model##Other##,Length##Length##Inches,Width##Length##Inches,Height##Length##Inches,Compressor Type##Other##,Refrigerant Used##Other##,Refrigerant Charge##Force##pounds,Compressor Quantity##Other##,Refrigerant Suction Gas Connection Diameter##pipe_size##Inches,Suction Gas Connection Offset Bottom##Length##Inches,Suction Gas Connection Offset Front##Length##Inches,Suction Gas Connection Offset Left##Length##Inches,Suction Gas 2 Connection Offset Left##Length##Inches,Suction Gas 2 Connection Offset Bottom##Length##Inches,Refrigerant Liquid Connection Diameter##pipe_size##Inches,Liquid Connection Offset Bottom##Length##Inches,Liquid 1 Connection Offset Front##Length##Inches,Liquid 1 Connection Offset Left##Length##Inches,Liquid 2 Connection Offset Front##Length##Inches,Liquid 2 Connection Offset Left##Length##Inches,Hot Gas Connection Diameter##pipe_size##Inches,Hot Gas Offset Left##Length##Inches,Hot Gas Offset Front##Length##Inches,Hot Gas Offset Bottom##Length##Inches,Hot Gas 2 Offset Left##Length##Inches,Base Rail Width##Length##Inches,Clearance Offset Top##Length##Inches,Clearance Offset Right##Length##Inches,Clearance Offset Left##Length##Inches,Clearance Offset Front##Length##Inches,Clearance Offset Bottom##Length##Inches,Clearance Offset Back##Length##Inches,Family Load Status##other##,Include Clearance##Other##
30 Ton,AGZ030E,94.3,88,94.8,SCROLL,R-410A,64,4,1.625,25.5,33.75,6.1,59.9,25.5,0.875,6.5,49.1,17.1,58.1,17.6,0.875,3,33.75,14.4,56.9,5.2,150,48,84,48,0,48,Valid – Type loaded via type catalog,1
35 Ton,AGZ035E,94.3,88,94.8,SCROLL,R-410A,70,4,1.625,25.5,33.75,6.1,59.9,25.5,0.875,6.5,49.1,17.1,58.1,17.6,0.875,3,33.75,14.4,56.9,5.2,150,48,84,48,0,48,Valid – Type loaded via type catalog,1
40 Ton,AGZ040E,94.3,88,94.8,SCROLL,R-410A,78,4,1.625,25.5,33.75,6.1,59.9,25.5,0.875,6.5,49.1,17.1,58.1,17.6,0.875,3,33.75,14.4,56.9,5.2,150,48,84,48,0,48,Valid – Type loaded via type catalog,1
45 Ton,AGZ045E,94.3,88,94.8,SCROLL,R-410A,88,4,1.625,25.5,33.75,6.1,59.9,25.5,0.875,6.5,49.1,17.1,58.1,17.6,0.875,3,33.75,14.4,56.9,5.2,150,48,84,48,0,48,Valid – Type loaded via type catalog,1
50 Ton,AGZ050E,94.3,88,94.8,SCROLL,R-410A,100,4,1.625,25.5,33.75,6.1,59.9,25.5,0.875,6.5,49.1,17.1,58.1,17.6,0.875,3,33.75,14.4,56.9,5.2,150,48,84,48,0,48,Valid – Type loaded via type catalog,1
55 Ton,AGZ055E,94.3,88,94.8,SCROLL,R-410A,104,4,1.625,25.5,33.75,6.1,59.9,25.5,0.875,6.5,49.1,17.1,58.1,17.6,0.875,3,33.75,14.4,56.9,5.2,150,48,84,48,0,48,Valid – Type loaded via type catalog,1
60 Ton,AGZ060E,94.3,88,94.8,SCROLL,R-410A,108,4,1.625,25.5,33.75,6.1,59.9,25.5,0.875,6.5,49.1,17.1,58.1,17.6,0.875,3,33.75,14.4,56.9,5.2,150,48,84,48,0,48,Valid – Type loaded via type catalog,1
65 Ton,AGZ065E,94.3,88,94.8,SCROLL,R-410A,116,4,1.625,25.5,33.75,6.1,59.9,25.5,0.875,6.5,49.1,17.1,58.1,17.6,0.875,3,33.75,14.4,56.9,5.2,150,48,84,48,0,48,Valid – Type loaded via type catalog,1
70 Ton,AGZ070E,94.3,88,94.8,SCROLL,R-410A,120,4,2.125,25.5,33.75,6.1,59.9,25.5,0.875,6.5,49.1,17.1,58.1,17.6,0.875,3,33.75,14.4,56.9,5.2,150,48,84,48,0,48,Valid – Type loaded via type catalog,1
