 ,Model##Other##,Length##Length##Inches,Width##Length##Inches,Height##Length##Inches,Compressor Type##Other##,Refrigerant Used##Other##,Compressor Quantity##Other##,Evaporator Diameter##Length##Inches,Evaporator Offset Bottom##Length##Inches,Evaporator Height##Length##Inches,Evaporator Offset Left##Length##Inches,Evaporator Supply Water Connection Diameter##Length##Inches,Evaporator Supply Water Connection Offset Right##Length##Inches,Evaporator Supply Water Connection Offset Bottom##Length##Inches,Evaporator Supply Water Connection Offset Front##Length##Inches,Evaporator Return Water Connection Offset Front##Length##Inches,Evaporator Return Water Connection Offset Right##Length##Inches,Evaporator Return Water Connection Diameter##Length##Inches,Evaporator Return Water Connection Offset Bottom##Length##Inches,Base Rail Width##Length##Inches,Clearance Offset Top##Length##Inches,Clearance Offset Right##Length##Inches,Clearance Offset Left##Length##Inches,Clearance Offset Front##Length##Inches,Clearance Offset Bottom##Length##Inches,Clearance Offset Back##Length##Inches,Family Load Status##other##,Include Clearance##Other##
75 Ton,AGZ075E,147,88,92.7,SCROLL,R-410A,4,20,6,30,60,4,32.5,11.4,44,58.7,39.6,4,22.3,5,150,48,48,48,0,96,Valid – Type loaded via type catalog,1
80 Ton,AGZ080E,147,88,92.7,SCROLL,R-410A,4,20,6,30,60,4,32.5,11.4,44,58.7,39.6,4,22.3,5,150,48,48,48,0,96,Valid – Type loaded via type catalog,1
90 Ton,AGZ090E,147,88,92.7,SCROLL,R-410A,4,20,6,30,60,4,32.5,11.4,44,58.7,39.6,4,22.3,5,150,48,48,48,0,96,Valid – Type loaded via type catalog,1
100 Ton,AGZ100E,147,88,92.7,SCROLL,R-410A,4,20,6,30,60,4,32.5,11.4,44,58.7,39.6,4,22.3,5,150,48,48,48,0,96,Valid – Type loaded via type catalog,1
