 ,Model##Other##,Length##Length##Inches,Width##Length##Inches,Height##Length##Inches,Compressor Type##Other##,Refrigerant Used##Other##,Compressor Quantity##Other##,Suction 1 Offset Front##Length##Inches,Suction 2 Offset Front##Length##Inches,Suction 1 Offset Bottom##Length##Inches,Refrigerant Suction Gas Diameter##pipe_size##inches,Evaporator Offset Bottom##Length##Inches,Evaporator Offset Front##Length##Inches,Evaporator Offset Left##Length##Inches,Evaporator Height##Length##Inches,Refrigerant Liquid 2 Connection Offset Front##Length##Inches,Refrigerant Liquid Connection Offset Front##Length##Inches,Refrigerant Liquid Connection Offset Bottom##Length##Inches,Refrigerant Suction Gas Connections Offset Left##Length##Inches,Refrigerant Liquid Connection Diameter##pipe_size##inches,Hot Gas Offset Bottom##Length##Inches,Hot Gas Connection Diameter##pipe_size##inches,Liquid and Hot Gas Connections Offset Left##Length##Inches,Base Rail Width##Length##Inches,Clearance Offset Top##Length##Inches,Clearance Offset Right##Length##Inches,Clearance Offset Left##Length##Inches,Clearance Offset Front##Length##Inches,Clearance Offset Bottom##Length##Inches,Clearance Offset Back##Length##Inches,Family Load Status##other##,Include Clearance##Other##
191 Ton,AGZ191E,282.3,88,92.7,SCROLL,R-410A,4,37,14,37.8,3.13,7,20,185,32.5,4.4,32.6,9,174.2,1.38,7.2,1.13,178.8,5.2,150,48,96,48,0,96,Valid – Type loaded via type catalog,1
211 Ton,AGZ211E,282.3,88,92.7,SCROLL,R-410A,4,37,14,37.8,3.13,7,20,185,32.5,4.4,32.6,9,174.2,1.38,7.2,1.13,178.8,5.2,150,48,96,48,0,96,Valid – Type loaded via type catalog,1
