 ,Model##Other##,Length##Length##Inches,Width##Length##Inches,Height##Length##Inches,Compressor Type##Other##,Refrigerant Used##Other##,Compressor Quantity##Other##,Evaporator Offset Bottom##Length##Inches,Evaporator Offset Front##Length##Inches,Evaporator Height##Length##Inches,Evaporator Offset Left##Length##Inches,Refrigerant Suction Gas Diameter##pipe_size##inches,Suction Gas Connection Offset Left##Length##Inches,Suction Gas Connection Offset Bottom##Length##Inches,Suction Gas 2 Connection Offset Front##Length##Inches,Suction Gas Connection Offset Front##Length##Inches,Liquid and Hot Gas Connection Offset Front##Length##Inches,Liquid Connection Offset Bottom##Length##Inches,Liquid and Hot Gas 2 Connection Offset Front##Length##Inches,Refrigerant Liquid Connection Diameter##pipe_size##inches,Hot Gas Connection Diameter##pipe_size##inches,Hot Gas Offset Bottom##Length##Inches,Base Rail Width##Length##Inches,Clearance Offset Top##Length##Inches,Clearance Offset Right##Length##Inches,Clearance Offset Left##Length##Inches,Clearance Offset Front##Length##Inches,Clearance Offset Bottom##Length##Inches,Clearance Offset Back##Length##Inches,Family Load Status##other##,Include Clearance##Other##
110 Ton,AGZ110E,192.1,88,92.7,SCROLL,R-410A,4,6,27,30,120,2.63,102.3,34.7,8,7.5,32.5,9,7.4,1.13,0.88,15.6,4,150,48,48,48,0,96,Valid – Type loaded via type catalog,1
120 Ton,AGZ120E,192.1,88,92.7,SCROLL,R-410A,4,6,27,30,120,2.63,102.3,34.7,8,7.5,32.5,9,7.4,1.13,0.88,15.6,4,150,48,48,48,0,96,Valid – Type loaded via type catalog,1
130 Ton,AGZ130E,192.1,88,92.7,SCROLL,R-410A,4,6,27,30,120,2.63,102.3,34.7,8,7.5,32.5,9,7.4,1.13,0.88,15.6,4,150,48,48,48,0,96,Valid – Type loaded via type catalog,1
