 ,Model##Other##,Length##Length##Inches,Width##Length##Inches,Height##Length##Inches,Refrigerant Used##Other##,Evaporator Water Connection Diameter##pipe_size##inches,Water Connection Between Connections##Length##Inches,Water Connection Offset Bottom##Length##Inches,Refrigerant Liquid Connection Diameter##pipe_size##inches,Liquid Connection Offset Bottom##Length##Inches,Liquid Connection Between Connections##Length##Inches,Water Connections Protrusion##Length##Inches,Refrigerant Suction Gas Connection Diameter##pipe_size##inches,Suction Gas Connection Offset Top##Length##Inches,Suction Gas Connection Between Connections##Length##Inches,Refrigerant Connections Protrusion##Length##Inches,Refrigerant Liquid Connections Protrusion##Length##Inches,Clearance Offset Top##Length##Inches,Clearance Offset Right##Length##Inches,Clearance Offset Left##Length##Inches,Clearance Offset Front##Length##Inches,Clearance Offset Bottom##Length##Inches,Clearance Offset Back##Length##Inches,Family Load Status##other##,Include Clearance##Other##
"191 Ton, for AGZ191EB",AGZ191EB,18.4,19.2,34.5,R-410A,5,24.21,6.13,1.63,8.1,11.02,1.97,3.13,2.66,14.02,2.05,1.18,12,12,12,12,0,12,Valid – Type loaded via type catalog,1
"211 Ton, for AGZ211EB",AGZ211EB,18.4,19.2,34.5,R-410A,5,24.21,6.13,1.63,8.1,11.02,1.97,3.13,2.66,14.02,2.05,1.18,12,12,12,12,0,12,Valid – Type loaded via type catalog,1
"226 Ton, for AGZ226EB",AGZ226EB,22.5,19.2,34.5,R-410A,5,24.21,6.13,1.63,8.1,11.02,1.97,3.13,2.66,14.02,2.05,1.18,12,12,12,12,0,12,Valid – Type loaded via type catalog,1
"241 Ton, for AGZ241EB",AGZ241EB,22.5,19.2,34.5,R-410A,5,24.21,6.13,1.63,8.1,11.02,1.97,3.13,2.66,14.02,2.05,1.18,12,12,12,12,0,12,Valid – Type loaded via type catalog,1
