 ,Model##Other##,Length##Length##Inches,Width##Length##Inches,Height##Length##Inches,Compressor Type##Other##,Refrigerant Used##Other##,Compressor Quantity##Other##,Evaporator Offset Front##Length##Inches,Evaporator Offset Bottom##Length##Inches,Evaporator Height##Length##Inches,Evaporator Offset Right##Length##Inches,Refrigerant Suction Gas Offset Front##Length##Inches,Refrigerant Suction Gas 2 Offset Front##Length##Inches,Refrigerant Suction Gas Offset Bottom##Length##Inches,Refrigerant Suction Gas Diameter##pipe_size##inches,Refrigerant Liquid Connection Diameter##pipe_size##inches,Refrigerant Liquid 2 Connection Offset Bottom##Length##Inches,Refrigerant Liquid Connection Offset Front##Length##Inches,Refrigerant Liquid 2 Connection Offset Front##Length##Inches,Connections Offset Left##Length##Inches,Hot Gas Offset Bottom##Length##Inches,Hot Gas Connection Diameter##pipe_size##inches,Base Rail Width##Length##Inches,Clearance Offset Top##Length##Inches,Clearance Offset Right##Length##Inches,Clearance Offset Left##Length##Inches,Clearance Offset Front##Length##Inches,Clearance Offset Bottom##Length##Inches,Clearance Offset Back##Length##Inches,Family Load Status##other##,Include Clearance##Other##
170 Ton,AGZ170E,237.2,88,92.7,SCROLL,R-410A,6,24,6,30,145,40,8,34.8,2.63,1.13,8.9,32.6,7.4,133.5,6.8,1.13,4,150,48,48,48,0,96,Valid – Type loaded via type catalog,1
180 Ton,AGZ180E,237.2,88,92.7,SCROLL,R-410A,6,24,6,30,145,40,8,34.8,2.63,1.13,8.9,32.6,7.4,133.5,6.8,1.13,4,150,48,48,48,0,96,Valid – Type loaded via type catalog,1
