 ,Model##Other##,Length##Length##Inches,Width##Length##Inches,Height##Length##Inches,Compressor Type##Other##,Refrigerant Used##Other##,Compressor Quantity##Other##,Evaporator Diameter##Length##Inches,Evaporator Offset Bottom##Length##Inches,Evaporator Height##Length##Inches,Evaporator Offset Left##Length##Inches,Evaporator Supply Water Connection Diameter##Length##Inches,Evaporator Supply Water Connection Offset Left##Length##Inches,Evaporator Supply Water Connection Offset Front##Length##Inches,Evaporator Supply Water Connection Offset Bottom##Length##Inches,Evaporator Return Water Connection Offset Left##Length##Inches,Evaporator Return Water Connection Diameter##Length##Inches,Evaporator Return Water Connection Offset Bottom##Length##Inches,Evaporator Return Water Connection Offset Front##Length##Inches,Base Rail Width##Length##Inches,Clearance Offset Top##Length##Inches,Clearance Offset Right##Length##Inches,Clearance Offset Left##Length##Inches,Clearance Offset Front##Length##Inches,Clearance Offset Bottom##Length##Inches,Clearance Offset Back##Length##Inches,Family Load Status##other##,Include Clearance##Other##
140 Ton,AGZ140E,237.2,88,92.7,SCROLL,R-410A,4,10,6,30,100,6,3.2,44,11.4,3.2,6,22.2,58.8,5,150,48,48,48,0,96,Valid – Type loaded via type catalog,1
150 Ton,AGZ150E,237.2,88,92.7,SCROLL,R-410A,4,10,6,30,100,6,3.2,44,11.4,3.2,6,22.2,58.8,5,150,48,48,48,0,96,Valid – Type loaded via type catalog,1
161 Ton,AGZ161E,237.2,88,92.7,SCROLL,R-410A,4,10,6,30,100,6,3.2,44,11.4,3.2,6,22.2,58.8,5,150,48,48,48,0,96,Valid – Type loaded via type catalog,1
