 ,Model##Other##,Length##Length##Inches,Width##Length##Inches,Height##Length##Inches,Compressor Type##Other##,Refrigerant Used##Other##,Compressor Quantity##Other##,Evaporator Supply Water Connection Diameter##Length##Inches,Evaporator Return Water Connection Diameter##Length##Inches,Evaporator Diameter##Length##Inches,Water Connection Offset Right##Length##Inches,Evaporator Offset Bottom##Length##Inches,Evaporator Offset Front##Length##Inches,Evaporator Offset Left##Length##Inches,Base Rail Width##Length##Inches,Evaporator Supply Water Connection Offset Left##Length##Inches,Evaporator Supply Water Connection Offset Bottom##Length##Inches,Evaporator Return Water Connection Offset Front##Length##Inches,Evaporator Supply Water Connection Offset Front##Length##Inches,Evaporator Return Water Connection Offset Left##Length##Inches,Evaporator Return Water Connection Offset Bottom##Length##Inches,Clearance Offset Top##Length##Inches,Clearance Offset Right##Length##Inches,Clearance Offset Left##Length##Inches,Clearance Offset Front##Length##Inches,Clearance Offset Bottom##Length##Inches,Clearance Offset Back##Length##Inches,Family Load Status##other##,Include Clearance##Other##
226 Ton,AGZ226E,327.45,88,92.7,SCROLL,R-410A,4,8,8,20,41.8,17,44,91,5,105.7,12.1,66,17.7,105.7,17.4,150,48,96,48,0,96,Valid – Type loaded via type catalog,1
241 Ton,AGZ241E,327.45,88,92.7,SCROLL,R-410A,4,8,8,20,41.8,17,44,91,5,105.7,12.1,66,17.7,105.7,17.4,150,48,96,48,0,96,Valid – Type loaded via type catalog,1
