 ,Model##Other##,Length##Length##Inches,Width##Length##Inches,Height##Length##Inches,Compressor Type##Other##,Refrigerant Used##Other##,Compressor Quantity##Other##,Evaporator Supply Water Connection Diameter##Length##Inches,Evaporator Return Water Connection Diameter##Length##Inches,Evaporator Diameter##Length##Inches,Water Connection Offset Right##Length##Inches,Evaporator Offset Bottom##Length##Inches,Evaporator Offset Front##Length##Inches,Evaporator Offset Left##Length##Inches,Base Rail Width##Length##Inches,Evaporator Supply Water Connection Offset Left##Length##Inches,Evaporator Supply Water Connection Offset Bottom##Length##Inches,Evaporator Return Water Connection Offset Front##Length##Inches,Evaporator Supply Water Connection Offset Front##Length##Inches,Evaporator Return Water Connection Offset Left##Length##Inches,Evaporator Return Water Connection Offset Bottom##Length##Inches,Clearance Offset Top##Length##Inches,Clearance Offset Right##Length##Inches,Clearance Offset Left##Length##Inches,Clearance Offset Front##Length##Inches,Clearance Offset Bottom##Length##Inches,Clearance Offset Back##Length##Inches,Family Load Status##other##,Include Clearance##Other##
225 Ton,AGZ225E,327.45,88,92.7,SCROLL,R-410A,4,8,8,16,3.4,17,44,97,5,105.7,17,66.4,10.8,216.4,17.4,150,48,96,48,0,96,Valid – Type loaded via type catalog,1
240 Ton,AGZ240E,327.45,88,92.7,SCROLL,R-410A,4,8,8,16,3.4,17,44,97,5,105.7,17,66.4,10.8,216.4,17.4,150,48,96,48,0,96,Valid – Type loaded via type catalog,1
