 ,Model##Other##,Length##Length##Inches,Width##Length##Inches,Height##Length##Inches,Compressor Type##Other##,Refrigerant Used##Other##,Compressor Quantity##Other##,Evaporator Offset Bottom##Length##Inches,Evaporator Offset Front##Length##Inches,Evaporator Offset Left##Length##Inches,Evaporator Height##Length##Inches,Suction 1 Offset Front##Length##Inches,Suction 2 Offset Front##Length##Inches,Suction 1 Offset Bottom##Length##Inches,Refrigerant Suction Connections Offset Left##Length##Inches,Refrigerant Suction Gas Diameter##pipe_size##inches,Refrigerant Liquid Connection Diameter##pipe_size##inches,Refrigerant Liquid Connection Offset Left##Length##Inches,Refrigerant Liquid Connection Offset Bottom##Length##Inches,Refrigerant Liquid Connection Offset Front##Length##Inches,Refrigerant Liquid Connection 2 Offset Front##Length##Inches,Hot Gas Offset Bottom##Length##Inches,Hot Gas Connection Diameter##pipe_size##inches,Base Rail Width##Length##Inches,Clearance Offset Top##Length##Inches,Clearance Offset Right##Length##Inches,Clearance Offset Left##Length##Inches,Clearance Offset Front##Length##Inches,Clearance Offset Bottom##Length##Inches,Clearance Offset Back##Length##Inches,Family Load Status##other##,Include Clearance##Other##
226 Ton,AGZ226E,327.45,88,92.7,SCROLL,R-410A,4,6,26,235,33.5,37,13.9,37.8,219.2,3.13,1.38,223.9,9,32.6,4.4,7.2,1.13,5.2,150,48,96,48,0,96,Valid – Type loaded via type catalog,1
241 Ton,AGZ241E,327.45,88,92.7,SCROLL,R-410A,4,6,26,235,33.5,37,13.9,37.8,219.2,3.13,1.38,223.9,9,32.6,4.4,7.2,1.13,5.2,150,48,96,48,0,96,Valid – Type loaded via type catalog,1
