 ,Model##Other##,Length##Length##Inches,Width##Length##Inches,Height##Length##Inches,Compressor Type##Other##,Refrigerant Used##Other##,Compressor Quantity##Other##,Evaporator Offset Bottom##Length##Inches,Evaporator Height##Length##Inches,Evaporator Offset Left##Length##Inches,Refrigerant Liquid Connection Diameter##pipe_size##inches,Liquid Connection Offset Bottom##Length##Inches,Liquid Connection Offset Front##Length##Inches,Liquid 2 Connection Offset Front##Length##Inches,Suction Gas Connection Offset Left##Length##Inches,Suction Gas Connection Offset Front##Length##Inches,Suction Gas Connection 2 Offset Front##Length##Inches,Suction Gas Connection Diameter##pipe_size##inches,Suction Gas Connection Offset Bottom##Length##Inches,Hot Gas Offset Bottom##Length##Inches,Hot Gas Offset Front##Length##Inches,Hot Gas 2 Offset Front##Length##Inches,Hot Gas Connection Diameter##pipe_size##inches,Base Rail Width##Length##Inches,Clearance Offset Top##Length##Inches,Clearance Offset Right##Length##Inches,Clearance Offset Left##Length##Inches,Clearance Offset Front##Length##Inches,Clearance Offset Bottom##Length##Inches,Clearance Offset Back##Length##Inches,Family Load Status##other##,Include Clearance##Other##
75 Ton,AGZ075E,147,88,92.7,SCROLL,R-410A,4,6,30,72,1.13,8.9,32.5,7.5,57.2,40,8.1,2.63,34.8,15.5,32.5,7.5,0.88,5.2,150,48,48,48,0,96,Valid – Type loaded via type catalog,1
80 Ton,AGZ080E,147,88,92.7,SCROLL,R-410A,4,6,30,72,1.13,8.9,32.5,7.5,57.2,40,8.1,2.63,34.8,15.5,32.5,7.5,0.88,5.2,150,48,48,48,0,96,Valid – Type loaded via type catalog,1
90 Ton,AGZ090E,147,88,92.7,SCROLL,R-410A,4,6,30,72,1.13,8.9,32.5,7.5,57.2,40,8.1,2.63,34.8,15.5,32.5,7.5,0.88,5.2,150,48,48,48,0,96,Valid – Type loaded via type catalog,1
100 Ton,AGZ100E,147,88,92.7,SCROLL,R-410A,4,6,30,72,1.13,8.9,32.5,7.5,57.2,40,8.1,2.63,34.8,15.5,32.5,7.5,0.88,5.2,150,48,48,48,0,96,Valid – Type loaded via type catalog,1
